diff --git a/drivers/gpu/drm/panel/Kconfig b/drivers/gpu/drm/panel/Kconfig
index b9dbedf8f..9a18418d8 100644
--- a/drivers/gpu/drm/panel/Kconfig
+++ b/drivers/gpu/drm/panel/Kconfig
@@ -499,4 +499,17 @@ config DRM_PANEL_XINPENG_XPP055C272
 	  Say Y here if you want to enable support for the Xinpeng
 	  XPP055C272 controller for 720x1280 LCD panels with MIPI/RGB/SPI
 	  system interfaces.
+
+config DRM_PANEL_CWD686
+	tristate "CWD686 panel"
+	depends on OF
+	depends on DRM_MIPI_DSI
+	depends on BACKLIGHT_CLASS_DEVICE
+	help
+	  Say Y here if you want to enable support for CWD686 panel.
+	  The panel has a 480x1280 resolution and uses 24 bit RGB per pixel.
+
+	  To compile this driver as a module, choose M here: the module
+	  will be called panel-cwd686.
+
 endmenu
diff --git a/drivers/gpu/drm/panel/Makefile b/drivers/gpu/drm/panel/Makefile
index 2ba560bca..80d40a803 100644
--- a/drivers/gpu/drm/panel/Makefile
+++ b/drivers/gpu/drm/panel/Makefile
@@ -53,3 +53,5 @@ obj-$(CONFIG_DRM_PANEL_TPO_TPG110) += panel-tpo-tpg110.o
 obj-$(CONFIG_DRM_PANEL_TRULY_NT35597_WQXGA) += panel-truly-nt35597.o
 obj-$(CONFIG_DRM_PANEL_VISIONOX_RM69299) += panel-visionox-rm69299.o
 obj-$(CONFIG_DRM_PANEL_XINPENG_XPP055C272) += panel-xinpeng-xpp055c272.o
+obj-$(CONFIG_DRM_PANEL_CWD686) += panel-cwd686.o
+
diff --git a/drivers/gpu/drm/panel/panel-cwd686.c b/drivers/gpu/drm/panel/panel-cwd686.c
new file mode 100644
index 000000000..6a0eabf92
--- /dev/null
+++ b/drivers/gpu/drm/panel/panel-cwd686.c
@@ -0,0 +1,283 @@
+// SPDX-License-Identifier: GPL-2.0+
+
+#include <drm/drm_modes.h>
+#include <drm/drm_mipi_dsi.h>
+#include <drm/drm_panel.h>
+#include <linux/backlight.h>
+#include <linux/gpio/consumer.h>
+#include <linux/regulator/consumer.h>
+#include <linux/delay.h>
+#include <linux/of_device.h>
+#include <linux/module.h>
+
+struct cwd686 {
+	struct device *dev;
+	struct drm_panel panel;
+	struct regulator *supply;
+	struct gpio_desc *enable_gpio;
+	struct gpio_desc *reset_gpio;
+	struct backlight_device *backlight;
+	bool prepared;
+	bool enabled;
+};
+
+static const struct drm_display_mode default_mode = {
+	.clock = 54465,
+	.hdisplay = 480,
+	.hsync_start = 480 + 150,
+	.hsync_end = 480 + 150 + 24,
+	.htotal = 480 + 150 + 24 + 40,
+	.vdisplay = 1280,
+	.vsync_start = 1280 + 12,
+	.vsync_end = 1280 + 12+ 6,
+	.vtotal = 1280 + 12 + 6 + 10,
+};
+
+static inline struct cwd686 *panel_to_cwd686(struct drm_panel *panel)
+{
+	return container_of(panel, struct cwd686, panel);
+}
+
+#define dcs_write_seq(seq...)                              \
+({                                                              \
+	static const u8 d[] = { seq };                          \
+	mipi_dsi_dcs_write_buffer(dsi, d, ARRAY_SIZE(d));	 \
+})
+
+static void cwd686_init_sequence(struct cwd686 *ctx)
+{
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+
+	dcs_write_seq(0xF0,0x5A,0x5A);
+	dcs_write_seq(0xF1,0xA5,0xA5);
+	dcs_write_seq(0xB6,0x0D,0x0D);
+	dcs_write_seq(0xB4,0x0A,0x08,0x12,0x10,0x0E,0x0C,0x00,0x00,0x00,0x03,0x00,0x03,0x03,0x03,0x03,0x03,0x03,0x03,0x04,0x06);
+	dcs_write_seq(0xB3,0x0B,0x09,0x13,0x11,0x0F,0x0D,0x00,0x00,0x00,0x03,0x00,0x03,0x03,0x03,0x03,0x03,0x03,0x03,0x05,0x07);
+	dcs_write_seq(0xB0,0x54,0x32,0x23,0x45,0x44,0x44,0x44,0x44,0x90,0x01,0x90,0x01);
+	dcs_write_seq(0xB1,0x32,0x84,0x02,0x83,0x30,0x01,0x6B,0x01);
+	dcs_write_seq(0xB2,0x73);
+	dcs_write_seq(0xBD,0x4E,0x0E,0x50,0x50,0x26,0x1D,0x00,0x14,0x42,0x03);
+	dcs_write_seq(0xB7,0x01,0x01,0x09,0x11,0x0D,0x55,0x19,0x19,0x21,0x1D,0x00,0x00,0x00,0x00,0x02,0xFF,0x3C);
+	dcs_write_seq(0xB8,0x23,0x01,0x30,0x34,0x63);
+	dcs_write_seq(0xB9,0xA0,0x22,0x00,0x44);
+	dcs_write_seq(0xBA,0x12,0x63);
+	dcs_write_seq(0xC1,0x0C,0x16,0x04,0x0C,0x10,0x04);
+	dcs_write_seq(0xC2,0x11,0x41);
+	dcs_write_seq(0xC3,0x22,0x31,0x04);
+	dcs_write_seq(0xC7,0x05,0x23,0x6B,0x49,0x00);
+	dcs_write_seq(0xC5,0x00);
+	dcs_write_seq(0xD0,0x37,0xFF,0xFF);
+	dcs_write_seq(0xD2,0x63,0x0B,0x08,0x88);
+	dcs_write_seq(0xD3,0x01,0x00,0x00,0x01,0x01,0x37,0x25,0x38,0x31,0x06,0x07);
+	dcs_write_seq(0xC8,0x7C,0x6A,0x5D,0x53,0x53,0x45,0x4B,0x35,0x4D,0x4A,0x49,0x66,0x53,0x57,0x4A,0x48,0x3B,0x2A,0x06,0x7C,0x6A,0x5D,0x53,0x53,0x45,0x4B,0x35,0x4D,0x4A,0x49,0x66,0x53,0x57,0x4A,0x48,0x3B,0x2A,0x06);//GAMMA2.2
+	dcs_write_seq(0xC6,0x00,0x00,0xFF,0x00,0x00,0xFF,0x00,0x00);
+	dcs_write_seq(0xF4,0x08,0x77);
+	dcs_write_seq(0x36,0x14);
+	dcs_write_seq(0x35,0x00);
+	dcs_write_seq(0xF1,0x5A,0x5A);
+	dcs_write_seq(0xF0,0xA5,0xA5);
+}
+
+static int cwd686_disable(struct drm_panel *panel)
+{
+	struct cwd686 *ctx = panel_to_cwd686(panel);
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+	int ret;
+
+	if (!ctx->enabled)
+		return 0;
+
+	backlight_disable(ctx->backlight);
+
+	ctx->enabled = false;
+
+	return 0;
+}
+
+static int cwd686_unprepare(struct drm_panel *panel)
+{
+	struct cwd686 *ctx = panel_to_cwd686(panel);
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+	int ret;
+
+#if 0
+	if (!ctx->prepared)
+		return 0;
+
+	ret = mipi_dsi_dcs_set_display_off(dsi);
+	if (ret) {
+		dev_err(ctx->dev, "failed to turn display off (%d)\n", ret);
+		return ret;
+	}
+	ret = mipi_dsi_dcs_enter_sleep_mode(dsi);
+	if (ret) {
+		dev_err(ctx->dev, "failed to enter sleep mode (%d)\n", ret);
+		return ret;
+	}
+
+	gpiod_set_value_cansleep(ctx->reset_gpio, 0);
+
+	ctx->prepared = false;
+#endif
+
+	return 0;
+}
+
+static int cwd686_prepare(struct drm_panel *panel)
+{
+	struct cwd686 *ctx = panel_to_cwd686(panel);
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+	int ret;
+
+	if (ctx->prepared)
+		return 0;
+
+	gpiod_set_value_cansleep(ctx->reset_gpio, 0);
+	msleep(10);
+	gpiod_set_value_cansleep(ctx->reset_gpio, 1);
+	msleep(120);
+
+	/* Enabe tearing mode: send TE (tearing effect) at VBLANK */
+	ret = mipi_dsi_dcs_set_tear_on(dsi, MIPI_DSI_DCS_TEAR_MODE_VBLANK);
+	if (ret) {
+		dev_err(ctx->dev, "failed to enable vblank TE (%d)\n", ret);
+		return ret;
+	}
+	/* Exit sleep mode and power on */
+
+	cwd686_init_sequence(ctx);
+
+	ret = mipi_dsi_dcs_exit_sleep_mode(dsi);
+	if (ret) {
+		dev_err(ctx->dev, "failed to exit sleep mode (%d)\n", ret);
+		return ret;
+	}
+	msleep(120);
+
+	ret = mipi_dsi_dcs_set_display_on(dsi);
+	if (ret) {
+		dev_err(ctx->dev, "failed to turn display on (%d)\n", ret);
+		return ret;
+	}
+	msleep(20);
+
+	ctx->prepared = true;
+
+	return 0;
+}
+
+static int cwd686_enable(struct drm_panel *panel)
+{
+	struct cwd686 *ctx = panel_to_cwd686(panel);
+	struct mipi_dsi_device *dsi = to_mipi_dsi_device(ctx->dev);
+	int ret;
+
+	if (ctx->enabled)
+		return 0;
+
+	backlight_enable(ctx->backlight);
+
+	ctx->enabled = true;
+
+	return 0;
+}
+
+static int cwd686_get_modes(struct drm_panel *panel, struct drm_connector *connector)
+{
+	struct drm_display_mode *mode;
+
+	mode = drm_mode_duplicate(connector->dev, &default_mode);
+	if (!mode) {
+		dev_err(panel->dev, "bad mode or failed to add mode\n");
+		return -EINVAL;
+	}
+	drm_mode_set_name(mode);
+	mode->type = DRM_MODE_TYPE_DRIVER | DRM_MODE_TYPE_PREFERRED;
+
+	connector->display_info.width_mm = mode->width_mm;
+	connector->display_info.height_mm = mode->height_mm;
+
+	drm_mode_probed_add(connector, mode);
+
+	return 1; /* Number of modes */
+}
+
+static const struct drm_panel_funcs cwd686_drm_funcs = {
+	.disable = cwd686_disable,
+	.unprepare = cwd686_unprepare,
+	.prepare = cwd686_prepare,
+	.enable = cwd686_enable,
+	.get_modes = cwd686_get_modes,
+};
+
+static int cwd686_probe(struct mipi_dsi_device *dsi)
+{
+	struct device *dev = &dsi->dev;
+	struct cwd686 *ctx;
+	int ret;
+
+	ctx = devm_kzalloc(dev, sizeof(*ctx), GFP_KERNEL);
+	if (!ctx)
+		return -ENOMEM;
+
+	mipi_dsi_set_drvdata(dsi, ctx);
+	ctx->dev = dev;
+
+	dsi->lanes = 4;
+	dsi->format = MIPI_DSI_FMT_RGB888;
+	dsi->mode_flags = MIPI_DSI_MODE_VIDEO |MIPI_DSI_MODE_VIDEO_BURST  | MIPI_DSI_MODE_VIDEO_SYNC_PULSE;
+
+	ctx->reset_gpio = devm_gpiod_get_optional(dev, "reset", GPIOD_OUT_HIGH);
+	if (IS_ERR(ctx->reset_gpio)) {
+		ret = PTR_ERR(ctx->reset_gpio);
+		if (ret != -EPROBE_DEFER)
+			dev_err(dev, "failed to request GPIO (%d)\n", ret);
+		return ret;
+	}
+
+	ctx->backlight = devm_of_find_backlight(dev);
+	if (IS_ERR(ctx->backlight))
+		return PTR_ERR(ctx->backlight);
+
+	drm_panel_init(&ctx->panel, dev, &cwd686_drm_funcs, DRM_MODE_CONNECTOR_DSI);
+
+	drm_panel_add(&ctx->panel);
+
+	ret = mipi_dsi_attach(dsi);
+	if (ret < 0) {
+		dev_err(dev, "mipi_dsi_attach() failed: %d\n", ret);
+		drm_panel_remove(&ctx->panel);
+		return ret;
+	}
+
+	return 0;
+}
+
+static int cwd686_remove(struct mipi_dsi_device *dsi)
+{
+	struct cwd686 *ctx = mipi_dsi_get_drvdata(dsi);
+
+	mipi_dsi_detach(dsi);
+	drm_panel_remove(&ctx->panel);
+
+	return 0;
+}
+
+static const struct of_device_id cwd686_of_match[] = {
+	{ .compatible = "cw,cwd686" },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, cwd686_of_match);
+
+static struct mipi_dsi_driver cwd686_driver = {
+	.probe = cwd686_probe,
+	.remove = cwd686_remove,
+	.driver = {
+		.name = "panel-cwd686",
+		.of_match_table = cwd686_of_match,
+	},
+};
+module_mipi_dsi_driver(cwd686_driver);
+
+MODULE_DESCRIPTION("DRM Driver for cwd686 MIPI DSI panel");
+MODULE_LICENSE("GPL v2");
diff --git a/drivers/gpu/drm/rockchip/dw-mipi-dsi-rockchip.c b/drivers/gpu/drm/rockchip/dw-mipi-dsi-rockchip.c
index 542dcf7ed..342a05834 100644
--- a/drivers/gpu/drm/rockchip/dw-mipi-dsi-rockchip.c
+++ b/drivers/gpu/drm/rockchip/dw-mipi-dsi-rockchip.c
@@ -692,13 +692,8 @@ static const struct dw_mipi_dsi_phy_ops dw_mipi_dsi_rockchip_phy_ops = {
 	.get_timing = dw_mipi_dsi_phy_get_timing,
 };
 
-static void dw_mipi_dsi_rockchip_config(struct dw_mipi_dsi_rockchip *dsi,
-					int mux)
+static void dw_mipi_dsi_rockchip_config(struct dw_mipi_dsi_rockchip *dsi)
 {
-	if (dsi->cdata->lcdsel_grf_reg)
-		regmap_write(dsi->grf_regmap, dsi->cdata->lcdsel_grf_reg,
-			mux ? dsi->cdata->lcdsel_lit : dsi->cdata->lcdsel_big);
-
 	if (dsi->cdata->lanecfg1_grf_reg)
 		regmap_write(dsi->grf_regmap, dsi->cdata->lanecfg1_grf_reg,
 					      dsi->cdata->lanecfg1);
@@ -712,6 +707,13 @@ static void dw_mipi_dsi_rockchip_config(struct dw_mipi_dsi_rockchip *dsi,
 					      dsi->cdata->enable);
 }
 
+static void dw_mipi_dsi_rockchip_set_lcdsel(struct dw_mipi_dsi_rockchip *dsi,
+					    int mux)
+{
+	regmap_write(dsi->grf_regmap, dsi->cdata->lcdsel_grf_reg,
+		mux ? dsi->cdata->lcdsel_lit : dsi->cdata->lcdsel_big);
+}
+
 static int
 dw_mipi_dsi_encoder_atomic_check(struct drm_encoder *encoder,
 				 struct drm_crtc_state *crtc_state,
@@ -767,9 +769,9 @@ static void dw_mipi_dsi_encoder_enable(struct drm_encoder *encoder)
 		return;
 	}
 
-	dw_mipi_dsi_rockchip_config(dsi, mux);
+	dw_mipi_dsi_rockchip_set_lcdsel(dsi, mux);
 	if (dsi->slave)
-		dw_mipi_dsi_rockchip_config(dsi->slave, mux);
+		dw_mipi_dsi_rockchip_set_lcdsel(dsi->slave, mux);
 
 	clk_disable_unprepare(dsi->grf_clk);
 }
@@ -923,6 +925,18 @@ static int dw_mipi_dsi_rockchip_bind(struct device *dev,
 		return ret;
 	}
 
+	ret = clk_prepare_enable(dsi->grf_clk);
+	if (ret) {
+		DRM_DEV_ERROR(dsi->dev, "Failed to enable grf_clk: %d\n", ret);
+		return ret;
+	}
+
+	dw_mipi_dsi_rockchip_config(dsi);
+	if (dsi->slave)
+		dw_mipi_dsi_rockchip_config(dsi->slave);
+
+	clk_disable_unprepare(dsi->grf_clk);
+
 	ret = rockchip_dsi_drm_create_encoder(dsi, drm_dev);
 	if (ret) {
 		DRM_DEV_ERROR(dev, "Failed to create drm encoder\n");
