## Step 1 {.step-title}
![FunKey and Screwdriver](/assets/images/IMG_8800.jpg){.step-thumb}
![Insert Screwdriver](/assets/images/IMG_8801.jpg){.step-thumb}
![Turn Screwdriver CCW](/assets/images/IMG_8802.jpg){.step-thumb}

 - You will need a Philips PH0 screwdriver
 - Insert the screwdriver in the hole
 - Turn the screwdriver counter-clockwise

## Step 2 {.step-title}
![FunKey screws and Screwdriver](/assets/images/IMG_8803.jpg){.step-thumb}
![FunKey and screws](/assets/images/IMG_8804.jpg){.step-thumb}

Now all the _screws_ are removed!

--8<--
includes/glossary.md
--8<--
