# This may not look like it, but it's a -*- makefile -*-
# sd2snes - SD card based universal cartridge for the SNES
# Copyright (C) 2009-2010 Maximilian Rehkopf <otakon@gmx.net>
#
# This file was adapted from sd2iec, written by Ingo Korb.
# Original disclaimer follows:
#
# sd2iec - SD/MMC to Commodore serial bus interface/controller
# Copyright (C) 2007-2009  Ingo Korb <ingo@akana.de>
#
# Inspiration and low-level SD/MMC access based on code from MMC2IEC
#   by Lars Pontoppidan et al., see sdcard.c|h and config.h.
#
#  FAT filesystem access based on code from ChaN, see tff.c|h.
#
#  This program is free software; you can redistribute it and/or modify
#  it under the terms of the GNU General Public License as published by
#  the Free Software Foundation; version 2 of the License only.
#
#  This program is distributed in the hope that it will be useful,
#  but WITHOUT ANY WARRANTY; without even the implied warranty of
#  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
#  GNU General Public License for more details.
#
#  You should have received a copy of the GNU General Public License
#  along with this program; if not, write to the Free Software
#  Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
#
#
# This file is included in the main sd2iec Makefile and also parsed
# into autoconf.h.

CONFIG_MCU=atmega644
CONFIG_LINKER_RELAX=n
CONFIG_MCU_FREQ=12288000
CONFIG_BOOTLOADER=y
CONFIG_BOOT_DEVID=0x4e534453
CONFIG_UART_DEBUG=y
CONFIG_UART_BAUDRATE=384000
CONFIG_UART_BUF_SHIFT=7
CONFIG_HARDWARE_NAME=sd2snes
CONFIG_SD_AUTO_RETRIES=10
#CONFIG_SD_DATACRC=y
CONFIG_EEPROM_SIZE=512
CONFIG_EEPROM_OFFSET=512
CONFIG_MAX_PARTITIONS=1
#CONFIG_DEADLOCK_ME_HARDER=y
