PCBNEW-BOARD Version 1 date 18/5/2009-17:20:42

$GENERAL
LayerCount 2
Ly 1FFF8001
Links 0
NoConn 0
Di 8440 7940 13560 13060
Ndraw 0
Ntrack 0
Nzone 0
Nmodule 2
Nnets 0
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "18 may 2009"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
UserGridSize 0.010000 0.010000 mm
ZoneGridSize 250
Layers 2
Layer[0] Copper signal
Layer[15] Component signal
TrackWidth 170
TrackWidthHistory 170
TrackClearence 60
ZoneClearence 150
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 450
ViaDrill 250
ViaSizeHistory 450
MicroViaSize 200
MicroViaDrill 80
MicroViasAllowed 0
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 600 600
PadDrill 320
AuxiliaryAxisOrg 0 0
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$MODULE PIN_ARRAY_5x2
Po 11000 12000 0 15 3FCF2109 4A11978A ~~
Li PIN_ARRAY_5x2
Cd Double rangee de contacts 2 x 5 pins
Kw CONN
Sc 4A11978A
AR /4A11978A
Op 0 0 0
T0 250 -1500 400 400 0 80 N V 21 "P102"
T1 0 -1500 400 400 0 80 N I 21 "CONN_5X2"
DS -2500 -1000 2500 -1000 120 21
DS 2500 -1000 2500 1000 120 21
DS 2500 1000 -2500 1000 120 21
DS -2500 1000 -2500 -1000 120 21
$PAD
Sh "1" R 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 500
$EndPAD
$PAD
Sh "2" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 -500
$EndPAD
$PAD
Sh "3" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 500
$EndPAD
$PAD
Sh "4" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 -500
$EndPAD
$PAD
Sh "5" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 500
$EndPAD
$PAD
Sh "6" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 -500
$EndPAD
$PAD
Sh "7" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 500
$EndPAD
$PAD
Sh "8" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 -500
$EndPAD
$PAD
Sh "9" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 500
$EndPAD
$PAD
Sh "10" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 -500
$EndPAD
$SHAPE3D
Na "pin_array/pins_array_5x2.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PIN_ARRAY_5x2
$MODULE PIN_ARRAY_5x2
Po 11000 9000 0 15 3FCF2109 4A119787 ~~
Li PIN_ARRAY_5x2
Cd Double rangee de contacts 2 x 5 pins
Kw CONN
Sc 4A119787
AR /4A119787
Op 0 0 0
T0 250 -1500 400 400 0 80 N V 21 "P101"
T1 0 -1500 400 400 0 80 N I 21 "CONN_5X2"
DS -2500 -1000 2500 -1000 120 21
DS 2500 -1000 2500 1000 120 21
DS 2500 1000 -2500 1000 120 21
DS -2500 1000 -2500 -1000 120 21
$PAD
Sh "1" R 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 500
$EndPAD
$PAD
Sh "2" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -2000 -500
$EndPAD
$PAD
Sh "3" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 500
$EndPAD
$PAD
Sh "4" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po -1000 -500
$EndPAD
$PAD
Sh "5" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 500
$EndPAD
$PAD
Sh "6" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 0 -500
$EndPAD
$PAD
Sh "7" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 500
$EndPAD
$PAD
Sh "8" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 1000 -500
$EndPAD
$PAD
Sh "9" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 500
$EndPAD
$PAD
Sh "10" C 600 600 0 0 0
Dr 400 0 0
At STD N 00E0FFFF
Ne 0 ""
Po 2000 -500
$EndPAD
$SHAPE3D
Na "pin_array/pins_array_5x2.wrl"
Sc 1.000000 1.000000 1.000000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  PIN_ARRAY_5x2
$TRACK
$EndTRACK
$ZONE
$EndZONE
$EndBOARD
