From 16aad5594e08550295ea3c12c1c9ed6f64774748 Mon Sep 17 00:00:00 2001
From: Rick Chen <rick@andestech.com>
Date: Tue, 29 Mar 2022 13:41:10 +0800
Subject: [PATCH] mmc: ftsdc010_mci: Support DTS of ftsdc010 driver for
 generic dma

The ftsdc010 driver has been implemented for generic dma in Linux
kernel. And its compatible is andestech,atfsdc010g to distinguish
the legacy andestech,atfsdc010 which is not for generic dma.

Althought the ftsdc010_mci driver in U-Boot does not use dma, but
it still can work well with the mmc node for generic dma. So add
the compatible string to support it.

Upstream-Status: Pending
Signed-off-by: Rick Chen <rick@andestech.com>
---
 drivers/mmc/ftsdc010_mci.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/mmc/ftsdc010_mci.c b/drivers/mmc/ftsdc010_mci.c
index 570d54cf9d..65b1d447a8 100644
--- a/drivers/mmc/ftsdc010_mci.c
+++ b/drivers/mmc/ftsdc010_mci.c
@@ -460,6 +460,7 @@ int ftsdc010_mmc_bind(struct udevice *dev)
 
 static const struct udevice_id ftsdc010_mmc_ids[] = {
 	{ .compatible = "andestech,atfsdc010" },
+	{ .compatible = "andestech,atfsdc010g" },
 	{ }
 };
 
-- 
2.34.1

