From 933ad8a59f7fd9b2088badc3e97167d750a40b5a Mon Sep 17 00:00:00 2001
From: Bin Meng <bmeng.cn@gmail.com>
Date: Mon, 12 Jul 2021 11:52:31 +0800
Subject: [PATCH] spl: Align device tree blob address at 8-byte boundary

Since libfdt v1.6.1, a new requirement on the device tree address via:

  commit 5e735860c478 ("libfdt: Check for 8-byte address alignment in fdt_ro_probe_()")

must be met that the device tree must be loaded in to memory at an
8-byte aligned address.

Upstream-Status: Pending
Signed-off-by: Bin Meng <bmeng.cn@gmail.com>
---
 common/spl/spl_fit.c | 6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/common/spl/spl_fit.c b/common/spl/spl_fit.c
index a35be529..a76ad14a 100644
--- a/common/spl/spl_fit.c
+++ b/common/spl/spl_fit.c
@@ -382,6 +382,12 @@ static int spl_fit_append_fdt(struct spl_image_info *spl_image,
 	 */
 	image_info.load_addr = spl_image->load_addr + spl_image->size;
 
+	/*
+	 * Since libfdt v1.6.1, the device tree must be loaded in to memory
+	 * at an 8-byte aligned address.
+	 */
+	image_info.load_addr = roundup(image_info.load_addr, 8);
+
 	/* Figure out which device tree the board wants to use */
 	node = spl_fit_get_image_node(ctx, FIT_FDT_PROP, index++);
 	if (node < 0) {
-- 
2.34.1

