diff --git a/config/boards/clockworkpi-a06.conf b/config/boards/clockworkpi-a06.conf
new file mode 100644
index 000000000..cb914d1c0
--- /dev/null
+++ b/config/boards/clockworkpi-a06.conf
@@ -0,0 +1,7 @@
+# Rockchip RK3399 hexa core 4GB RAM SoC WiFi/BT
+BOARD_NAME="Clockworkpi A06"
+BOARDFAMILY="rk3399"
+BOOTCONFIG="clockworkpi-a06-rk3399_defconfig"
+KERNEL_TARGET="legacy,current,edge"
+FULL_DESKTOP="yes"
+BOOT_LOGO="desktop"
diff --git a/config/kernel/linux-rockchip64-current.config b/config/kernel/linux-rockchip64-current.config
index a777730db..891a37384 100644
--- a/config/kernel/linux-rockchip64-current.config
+++ b/config/kernel/linux-rockchip64-current.config
@@ -4405,8 +4405,8 @@ CONFIG_MFD_AAT2870_CORE=y
 # CONFIG_MFD_BCM590XX is not set
 # CONFIG_MFD_BD9571MWV is not set
 CONFIG_MFD_AC100=m
-CONFIG_MFD_AXP20X=m
-# CONFIG_MFD_AXP20X_I2C is not set
+CONFIG_MFD_AXP20X=y
+CONFIG_MFD_AXP20X_I2C=y
 CONFIG_MFD_AXP20X_RSB=m
 CONFIG_MFD_CROS_EC_DEV=y
 # CONFIG_MFD_MADERA is not set
@@ -4521,7 +4521,7 @@ CONFIG_REGULATOR_88PG86X=m
 CONFIG_REGULATOR_AAT2870=m
 CONFIG_REGULATOR_AS3711=m
 CONFIG_REGULATOR_AS3722=m
-CONFIG_REGULATOR_AXP20X=m
+CONFIG_REGULATOR_AXP20X=y
 CONFIG_REGULATOR_BD70528=m
 CONFIG_REGULATOR_BD71828=m
 # CONFIG_REGULATOR_CROS_EC is not set
@@ -5470,6 +5470,7 @@ CONFIG_DRM_PANEL_TPO_TPG110=m
 CONFIG_DRM_PANEL_TRULY_NT35597_WQXGA=m
 # CONFIG_DRM_PANEL_VISIONOX_RM69299 is not set
 CONFIG_DRM_PANEL_XINPENG_XPP055C272=m
+CONFIG_DRM_PANEL_CWD686=m
 # end of Display Panels
 
 CONFIG_DRM_BRIDGE=y
@@ -5645,6 +5646,7 @@ CONFIG_BACKLIGHT_GPIO=m
 # CONFIG_BACKLIGHT_ARCXCNN is not set
 CONFIG_BACKLIGHT_RAVE_SP=m
 CONFIG_BACKLIGHT_LED=m
+CONFIG_BACKLIGHT_OCP8178=m
 # end of Backlight & LCD device support
 
 CONFIG_VIDEOMODE_HELPERS=y
@@ -5939,6 +5941,7 @@ CONFIG_SND_SOC_HDMI_CODEC=m
 CONFIG_SND_SOC_ES7134=m
 CONFIG_SND_SOC_ES7241=m
 CONFIG_SND_SOC_ES8316=m
+CONFIG_SND_SOC_ES8323=m
 CONFIG_SND_SOC_ES8328=m
 CONFIG_SND_SOC_ES8328_I2C=m
 CONFIG_SND_SOC_ES8328_SPI=m
