(footprint "EP_DEV_PORT"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Exposed DSpico Development port")
	(property "Reference" "REF**"
		(at 6.35 -1.75 0)
		(layer "F.SilkS")
		(uuid "9f6a29e4-f260-47df-9811-f044dba175aa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "EP_DEV_PORT"
		(at 6.35 1.75 0)
		(layer "F.Fab")
		(uuid "08a81d50-0de7-45d6-91eb-871d88d2828f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "919441bb-9ded-472b-8ecd-6f87f283edcf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1a2f2af8-b754-4951-add7-657a12efa83c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "SWD"
		(at 0.39802 0.9673 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "12c1681e-5b0b-401c-bd08-7063e6f19a61")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(fp_text user "SWCLK"
		(at 2.93802 0.96729 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "488aea22-7fe2-4d51-a70a-6fcd2581dc37")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(fp_text user "3V3"
		(at 5.47802 0.9673 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f7e76cbf-9cab-436d-8c69-6c3c014d3a64")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(fp_text user "TX0"
		(at 8.01802 0.9673 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "861e3cca-65ee-43b5-a2c5-b894a0a4425e")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(fp_text user "RX0"
		(at 10.55802 0.9673 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1a90a9de-4be9-4c3d-a050-f88127770c1a")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(fp_text user "GND"
		(at 13.09802 0.9673 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fc821dfa-1d10-49d1-8111-5bea82f5ece1")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.2)
			)
			(justify right bottom)
		)
	)
	(pad "1" smd rect
		(at 0 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "1a059575-7f1b-44c8-8d16-337bf0067568")
	)
	(pad "2" smd rect
		(at 2.54 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "b2a909fe-e098-44c4-aebc-1126ae05881c")
	)
	(pad "3" smd rect
		(at 5.08 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "3ccdeca0-d99b-4e65-9069-7ea677c755e9")
	)
	(pad "4" smd rect
		(at 7.62 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "e7cbf62a-d60b-4a35-ad52-4b5e40c6e1df")
	)
	(pad "5" smd rect
		(at 10.16 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "abfb4219-eb97-4c3c-8cae-b42a92034bdd")
	)
	(pad "6" smd rect
		(at 12.7 0 90)
		(size 2.1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1)
		(uuid "e04d95bd-23ec-4bd0-8e88-cf4550ba57bc")
	)
	(embedded_fonts no)
)
