(export (version D)
  (design
    (source FunKey.sch)
    (date "ven. 27 nov. 2020 23:48:42")
    (tool "Eeschema 5.1.5+dfsg1-2build2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title FunKey)
        (company "© 2017-2020 Michel Stempin, All rights reserved.")
        (rev E)
        (date 2020/11/26)
        (source FunKey.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U5)
      (value AXP209)
      (footprint FunKey:QFN48)
      (fields
        (field (name PARTNO) AXP209))
      (libsource (lib FunKey) (part AXP20) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A8DFD068))
    (comp (ref L3)
      (value 74404032047)
      (footprint FunKey:WE-LQS)
      (fields
        (field (name INDUCTANCE) 4.7uH)
        (field (name PARTNO) 74404032047)
        (field (name RATE) 1.2A)
        (field (name SIZE) 1208)
        (field (name TOL) ±20%))
      (libsource (lib FunKey) (part 74404032047) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 16675DB9))
    (comp (ref L4)
      (value 74404032047)
      (footprint FunKey:WE-LQS)
      (fields
        (field (name INDUCTANCE) 4.7uH)
        (field (name PARTNO) 74404032047)
        (field (name RATE) 1.2A)
        (field (name TOL) ±20%))
      (libsource (lib FunKey) (part 74404032047) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp AC177953))
    (comp (ref R24)
      (value 10k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp AE0241E3))
    (comp (ref C78)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F97CABE))
    (comp (ref C75)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 68A5AC33))
    (comp (ref C70)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C1F60F11))
    (comp (ref C67)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 4418D93E))
    (comp (ref R22)
      (value 200k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_200k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1278074E))
    (comp (ref C64)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CC2FA002))
    (comp (ref C52)
      (value 4u7)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_4u7_X5R_10%_CER_10V)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 10V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9BA5F96A))
    (comp (ref C55)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6E536519))
    (comp (ref R18)
      (value 1k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_1k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9886751E))
    (comp (ref C42)
      (value 100p)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100p_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A71B8181))
    (comp (ref R17)
      (value 47k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_47k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EA1BEB0F))
    (comp (ref R13)
      (value 10k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp DEE37B10))
    (comp (ref R14)
      (value 2k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_2k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EB687608))
    (comp (ref R16)
      (value 2k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_2k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1B61C57A))
    (comp (ref R15)
      (value 47k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_47k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B066BDBD))
    (comp (ref C33)
      (value 4u7)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_4u7_X5R_10%_CER_10V)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 10V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 336ED45C))
    (comp (ref C63)
      (value 4u7)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_4u7_X5R_10%_CER_10V)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 10V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7221EA1D))
    (comp (ref C69)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3C4D8EE3))
    (comp (ref C38)
      (value 4u7)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_4u7_X5R_10%_CER_10V)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 10V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 75EDD028))
    (comp (ref C72)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3AEF50EC))
    (comp (ref C30)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F1356F80))
    (comp (ref C34)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AF78AA4))
    (comp (ref C39)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A29482CB))
    (comp (ref C43)
      (value 1n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1n_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 026EFC73))
    (comp (ref C26)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B33389F0))
    (comp (ref C29)
      (value 1n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1n_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 88B5AEAA))
    (comp (ref C53)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 44149116))
    (comp (ref C60)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0EF3DB40))
    (comp (ref C56)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp DDAE881F))
    (comp (ref C59)
      (value 4u7)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_4u7_X5R_10%_CER_10V)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 10V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 69019886))
    (comp (ref R21)
      (value 30m)
      (footprint FunKey:R0603)
      (fields
        (field (name PARTNO) R0603_30m_1%_333mW)
        (field (name RATE) 333mW)
        (field (name SIZE) 0603)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0603) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9D9E9DF6))
    (comp (ref U4)
      (value SY8088AAC)
      (footprint FunKey:SOT23-5)
      (fields
        (field (name PARTNO) SY8088AAC))
      (libsource (lib FunKey) (part SY8088AAC) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7C57E89D))
    (comp (ref R20)
      (value 200k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_200k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp FEB6C18A))
    (comp (ref R23)
      (value 100k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_100k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 8DCB80EF))
    (comp (ref R19)
      (value 100k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_100k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp FCBADD89))
    (comp (ref C65)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3F458A12))
    (comp (ref C37)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 93A7D353))
    (comp (ref C73)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 21D5509F))
    (comp (ref L6)
      (value WPN201610U2R2NT)
      (footprint FunKey:L1008)
      (fields
        (field (name PARTNO) L1008)
        (field (name RATE) 1.2A)
        (field (name TOL) ±20%))
      (libsource (lib FunKey) (part L1008-) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5655E003))
    (comp (ref C24)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C533F2EC))
    (comp (ref C44)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 650F53C5))
    (comp (ref C46)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1C391E83))
    (comp (ref C48)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6D8FE889))
    (comp (ref C61)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp ABB13794))
    (comp (ref C77)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp E05ADCA6))
    (comp (ref C22)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 66C8AD90))
    (comp (ref C36)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CB733952))
    (comp (ref C41)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 452A4F92))
    (comp (ref C49)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±1V0%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 816363F5))
    (comp (ref C51)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 37105C01))
    (comp (ref C45)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp D97F1696))
    (comp (ref C71)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3F927A1A))
    (comp (ref C76)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp BAA894CD))
    (comp (ref C80)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9F450337))
    (comp (ref C82)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 47276C84))
    (comp (ref C21)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 30F436E8))
    (comp (ref C19)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 648C00B4))
    (comp (ref C40)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7749E55A))
    (comp (ref C35)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 65EDC034))
    (comp (ref C20)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 247FF2DC))
    (comp (ref C16)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7A36C4F5))
    (comp (ref C68)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B1C3D14))
    (comp (ref C27)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 29E2B3A1))
    (comp (ref C31)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59F5116A))
    (comp (ref C17)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A003222B))
    (comp (ref C58)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 207C652E))
    (comp (ref C62)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 965F3FF0))
    (comp (ref C66)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0DADD08D))
    (comp (ref C57)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp DE884EB4))
    (comp (ref C74)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp D84DC28E))
    (comp (ref C79)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 106EAFD2))
    (comp (ref C81)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 08B1EF11))
    (comp (ref R25)
      (value 2k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_2k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A6B2995B))
    (comp (ref R28)
      (value 2k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_2k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EFDBCC36))
    (comp (ref R11)
      (value 240R)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_240R_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2A2E4A68))
    (comp (ref R6)
      (value 200k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_200k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CDBFD3F3))
    (comp (ref C9)
      (value 1n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1n_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CB0C19C6))
    (comp (ref R4)
      (value 47k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_47k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A9BE52EE))
    (comp (ref C8)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp FA2D35D6))
    (comp (ref C10)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp BF98E6C5))
    (comp (ref C6)
      (value 1n)
      (footprint FunKey:C1206)
      (fields
        (field (name PARTNO) C1206_1n_X7R_10%_CER_500V)
        (field (name SIZE) 1206)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 500V))
      (libsource (lib FunKey) (part CAP_1206) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1283B2EE))
    (comp (ref L2)
      (value CBM321609U601T)
      (footprint FunKey:FB1206)
      (fields
        (field (name OPT) 600R/2A)
        (field (name PARTNO) FB1206_600R_25%)
        (field (name SIZE) 1206))
      (libsource (lib FunKey) (part FB_1206) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6CA6780F))
    (comp (ref C7)
      (value 10n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10n_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9A8C1A8D))
    (comp (ref D15)
      (value PRTR5V0U2X,215)
      (footprint FunKey:SOT143B)
      (fields
        (field (name PARTNO) PRTR5V0U2X,215))
      (libsource (lib FunKey) (part PRTR5V0U2X,215) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2A336CCE))
    (comp (ref D16)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2401D5E8))
    (comp (ref D17)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2F2D2D46))
    (comp (ref D18)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp AD6C63E9))
    (comp (ref D25)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 579BF510))
    (comp (ref D26)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EC83C2BC))
    (comp (ref D27)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5A34A7E8))
    (comp (ref D28)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp BA5CEA8D))
    (comp (ref R2)
      (value 100k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_100k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1452DE6A))
    (comp (ref C5)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61218984))
    (comp (ref L1)
      (value GZ1608D601CTF)
      (footprint FunKey:FB0603)
      (fields
        (field (name OPT) 600R)
        (field (name PARTNO) FB0603_600R_25%)
        (field (name RATE) 0.5A)
        (field (name SIZE) 0603))
      (libsource (lib FunKey) (part FB_0603) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B34A3BBA))
    (comp (ref Y2)
      (value K-F-24.000M-18-1010-2070-40)
      (footprint FunKey:CRYSTAL_32X25)
      (fields
        (field (name CAP) "18 pF")
        (field (name FREQ) "24 MHz")
        (field (name PARTNO) XTAL3225_4P_24M_18PF_10PPM)
        (field (name TOL) "10 ppm"))
      (libsource (lib FunKey) (part CRYSTAL_2SH) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 67C8FD8A))
    (comp (ref C12)
      (value 18pF)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_18p_NP0_5%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) NP0)
        (field (name TOL) ±5%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 245326F5))
    (comp (ref C13)
      (value 18pF)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_18p_NP0_5%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) NP0)
        (field (name TOL) ±5%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EC8D3AE2))
    (comp (ref C15)
      (value 18pF)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_18p_NP0_5%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) NP0)
        (field (name TOL) ±5%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EB999848))
    (comp (ref Y1)
      (value "FC-12M 32.768000kHz 12.5 +20.0-20.0")
      (footprint FunKey:FC-12M)
      (fields
        (field (name CAP) 12.5pF)
        (field (name FREQ) "32.768 kHz")
        (field (name PARTNO) FC-12M_32K768_12.5PF_20PPM)
        (field (name TOL) "20 ppm"))
      (libsource (lib FunKey) (part FC-12M) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 10584126))
    (comp (ref R12)
      (value 10M)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10M_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3B7D3F7E))
    (comp (ref R8)
      (value 33R)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_33R_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3216DFB6))
    (comp (ref C54)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp ED38BD29))
    (comp (ref R3)
      (value 1k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_1k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp D483747B))
    (comp (ref R26)
      (value 10k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 49EEB110))
    (comp (ref D30)
      (value BLUE)
      (footprint FunKey:LED0402)
      (fields
        (field (name PARTNO) LED0402-BLUE)
        (field (name SIZE) 0402))
      (libsource (lib FunKey) (part LED_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A3C75EF9))
    (comp (ref R9)
      (value 2R2)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_2R2_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp BE9409BB))
    (comp (ref C11)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C1573C9E))
    (comp (ref C18)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6BB2805E))
    (comp (ref R7)
      (value 4k7)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_4k7_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7C827D6A))
    (comp (ref R5)
      (value 1k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_1k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F5E59E3A))
    (comp (ref C28)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1AF00DE7))
    (comp (ref C32)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B6B40699))
    (comp (ref C47)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1EC6C39A))
    (comp (ref D29)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 78B73F3E))
    (comp (ref S13)
      (value EVP-BB)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB2A9B000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 206AFE7C))
    (comp (ref J2)
      (value U02-BFD3111B0-009)
      (footprint FunKey:U02-BFD3111B0-009)
      (fields
        (field (name PARTNO) U02-BFD3111B0-009))
      (libsource (lib FunKey) (part U02-BFD3111B0-009) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F2D55355))
    (comp (ref U2)
      (value PAM8301AAF)
      (footprint FunKey:TSOT26)
      (fields
        (field (name PARTNO) PAM8301AAF))
      (libsource (lib FunKey) (part PAM8301AAF) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C2DEB937))
    (comp (ref C4)
      (value 1u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_1u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 114A7209))
    (comp (ref C3)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0AE61553))
    (comp (ref D31)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F08F376B))
    (comp (ref D24)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 55A6EED1))
    (comp (ref D23)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F372D97))
    (comp (ref D22)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 52FDD551))
    (comp (ref D21)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp ABC76AEC))
    (comp (ref D20)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 55F32469))
    (comp (ref D19)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 94D7F43E))
    (comp (ref D14)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1D9EF25F))
    (comp (ref D13)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 141256B4))
    (comp (ref R1)
      (value 10k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B9BAFB95))
    (comp (ref C1)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 218CB388))
    (comp (ref C2)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 69098DAB))
    (comp (ref D1)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 8299ABF0))
    (comp (ref D2)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2FCA3BB7))
    (comp (ref D3)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 361BCA0E))
    (comp (ref D4)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp D3685E79))
    (comp (ref D7)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6B2274FC))
    (comp (ref D12)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 28136419))
    (comp (ref D11)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B54A8A3B))
    (comp (ref D10)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 4135B388))
    (comp (ref D9)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0E74ED9B))
    (comp (ref D6)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 03257839))
    (comp (ref S8)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9C0D287F))
    (comp (ref S9)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 293A7483))
    (comp (ref S10)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C58706E9))
    (comp (ref S11)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 768122A5))
    (comp (ref S3)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B30B70E4))
    (comp (ref S4)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F9C865EA))
    (comp (ref S5)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp B36A1E9D))
    (comp (ref S6)
      (value EVP-BB1AAB000)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB1AAB000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EC2185E0))
    (comp (ref S1)
      (value EVP-BB)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB2A9B000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CEBFFD5E))
    (comp (ref S2)
      (value EVP-BB)
      (footprint FunKey:EVP-BB)
      (fields
        (field (name PARTNO) EVP-BB2A9B000))
      (libsource (lib FunKey) (part EVP-BB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F82F9BF5))
    (comp (ref J1)
      (value MH3-1-0.05)
      (footprint FunKey:MH3-1-0.05)
      (fields
        (field (name DNP) T)
        (field (name PARTNO) MH3-1-0.05))
      (libsource (lib FunKey) (part MH3-1-0.05) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2CE6A523))
    (comp (ref J5)
      (value SM02B-SRSS-TB)
      (footprint FunKey:SM02B-SRSS-TB)
      (fields
        (field (name PARTNO) SM02B-SRSS-TB))
      (libsource (lib FunKey) (part SM02B-SRSS-TB) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0A445BA9))
    (comp (ref SP1)
      (value CDM-10008)
      (footprint FunKey:CDM-10008)
      (fields
        (field (name PARTNO) CDM-10008)
        (field (name RATE) 0.5W))
      (libsource (lib FunKey) (part CDM-10008) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 8A50F2F1))
    (comp (ref TP1)
      (value RESET)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp BB1D2254))
    (comp (ref TP2)
      (value PMU)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 66D3A59F))
    (comp (ref TP3)
      (value SDA)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C29349A6))
    (comp (ref TP4)
      (value SCL)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 44986D3A))
    (comp (ref TP5)
      (value C/D)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1DADCB0C))
    (comp (ref TP6)
      (value CLK)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 67489C2B))
    (comp (ref TP7)
      (value MOSI)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 661D6B70))
    (comp (ref TP8)
      (value CS)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EA795974))
    (comp (ref TP10)
      (value KEY)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C1FACBAD))
    (comp (ref TP11)
      (value PA)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6E86AACE))
    (comp (ref TP12)
      (value HP)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6698615D))
    (comp (ref TP13)
      (value +1V25)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 629E1F07))
    (comp (ref TP14)
      (value +3V3)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp FD82F57D))
    (comp (ref TP15)
      (value +AO)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BF494AB))
    (comp (ref TP16)
      (value +1V8)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 4B94CC33))
    (comp (ref TP17)
      (value +3V0)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 8E92EEBF))
    (comp (ref TP19)
      (value +VUSB)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 039021F4))
    (comp (ref TP20)
      (value +VBAT)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CEC9CD84))
    (comp (ref TP21)
      (value CHG)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 474643C3))
    (comp (ref TP22)
      (value POWER)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 129DF4A7))
    (comp (ref TP23)
      (value +VOUT)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 716AB1C5))
    (comp (ref F1)
      (value FIDUCIAL)
      (footprint FunKey:FIDUCIAL)
      (libsource (lib FunKey) (part FIDUCIAL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CDD216A9))
    (comp (ref F2)
      (value FIDUCIAL)
      (footprint FunKey:FIDUCIAL)
      (libsource (lib FunKey) (part FIDUCIAL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3F277CF6))
    (comp (ref F3)
      (value FIDUCIAL)
      (footprint FunKey:FIDUCIAL)
      (libsource (lib FunKey) (part FIDUCIAL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp DDB055F8))
    (comp (ref F4)
      (value FIDUCIAL)
      (footprint FunKey:FIDUCIAL)
      (libsource (lib FunKey) (part FIDUCIAL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 53CFCF21))
    (comp (ref Q1)
      (value IRLML2244TRPBF)
      (footprint FunKey:SOT23-3)
      (fields
        (field (name PARTNO) IRLML2244TRPBF))
      (libsource (lib FunKey) (part IRLML2244TRPBF) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7A211019))
    (comp (ref R29)
      (value 47k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_47k_5%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 5%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp AFE325EC))
    (comp (ref TP18)
      (value LCDR)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6C696087))
    (comp (ref S14)
      (value MK24-A-3)
      (footprint FunKey:MK24)
      (fields
        (field (name PARTNO) MK24-A-3))
      (libsource (lib FunKey) (part MK24--?3) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp E55EDFAE))
    (comp (ref C83)
      (value 100p)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100p_X7R_10%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 39538D82))
    (comp (ref J4)
      (value TF-110)
      (footprint FunKey:TF-110)
      (fields
        (field (name PARTNO) TF-110))
      (libsource (lib FunKey) (part TF-110) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2A89DB3B))
    (comp (ref TP24)
      (value LEDA)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EE31EC61))
    (comp (ref TP9)
      (value NOE)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CD04EBA2))
    (comp (ref TP25)
      (value GND)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp CCC12BEC))
    (comp (ref TP26)
      (value D-)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9A4D3F76))
    (comp (ref TP27)
      (value D+)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp A76606F2))
    (comp (ref TP28)
      (value D1)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 3D5E4C5A))
    (comp (ref TP29)
      (value D0)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1CF15E62))
    (comp (ref TP30)
      (value CLK)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 00634F2B))
    (comp (ref TP31)
      (value CMD)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 4D52FAC0))
    (comp (ref TP32)
      (value D3)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 2CF563B3))
    (comp (ref TP33)
      (value D2)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp E56B7C31))
    (comp (ref D32)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 46FC39B5))
    (comp (ref TP34)
      (value TE)
      (footprint FunKey:TEST_PAD)
      (libsource (lib FunKey) (part TEST_PAD) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp DA05B875))
    (comp (ref S12)
      (value EVP-AE)
      (footprint FunKey:EVP-AE)
      (fields
        (field (name PARTNO) EVP-AE))
      (libsource (lib FunKey) (part EVP-AE) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 78FF35FA))
    (comp (ref S7)
      (value EVP-AE)
      (footprint FunKey:EVP-AE)
      (fields
        (field (name PARTNO) EVP-AE))
      (libsource (lib FunKey) (part EVP-AE) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 98C882A3))
    (comp (ref U1)
      (value PCAL6416AHF,128)
      (footprint FunKey:QFN24)
      (fields
        (field (name PARTNO) PCAL6416AHF,128))
      (libsource (lib FunKey) (part PCAL6416A?,128HF) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F9562130))
    (comp (ref J3)
      (value DF37NB-24DS-0.4V)
      (footprint FunKey:DF37NB-24DS-0.4V)
      (fields
        (field (name PARTNO) DF37NB-24DS-0.4V))
      (libsource (lib FunKey) (part DF37NB-24DS-0.4V) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp D6A0AFFD))
    (comp (ref C25)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 1DB35DCC))
    (comp (ref C50)
      (value 100n)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_100n_X7R_10%_CER_16V)
        (field (name SIZE) 0402)
        (field (name TC) X7R)
        (field (name TOL) ±10%)
        (field (name TYPE) CER)
        (field (name VOLT) 16V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 037FE3C3))
    (comp (ref U3)
      (value V3S)
      (footprint FunKey:ELQFP-128)
      (libsource (lib FunKey) (part V3S) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 9A04CEE8))
    (comp (ref C14)
      (value 18pF)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_18p_NP0_5%_CER_50V)
        (field (name SIZE) 0402)
        (field (name TC) NP0)
        (field (name TOL) ±5%)
        (field (name TYPE) CER)
        (field (name VOLT) 50V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0858F80E))
    (comp (ref R27)
      (value 200k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_200k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp C362DB0F))
    (comp (ref D5)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 7C3AB992))
    (comp (ref D8)
      (value ESD5311N-2/TR)
      (footprint FunKey:ESD0402)
      (fields
        (field (name PARTNO) ESD0402_5V5_BIDIR)
        (field (name SIZE) 0402)
        (field (name VOLT) 6V))
      (libsource (lib FunKey) (part ESD0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp F92A98F9))
    (comp (ref R10)
      (value 10k)
      (footprint FunKey:R0402)
      (fields
        (field (name PARTNO) R0402_10k_1%_62.5mW)
        (field (name RATE) 62.5mW)
        (field (name SIZE) 0402)
        (field (name TOL) 1%))
      (libsource (lib FunKey) (part RES_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 0A067037))
    (comp (ref C23)
      (value 10u)
      (footprint FunKey:C0402)
      (fields
        (field (name PARTNO) C0402_10u_X5R_20%_CER_6V3)
        (field (name SIZE) 0402)
        (field (name TC) X5R)
        (field (name TOL) ±20%)
        (field (name TYPE) CER)
        (field (name VOLT) 6.3V))
      (libsource (lib FunKey) (part CAP_0402) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp EA0EB25A))
    (comp (ref L5)
      (value 74404032047)
      (footprint FunKey:WE-LQS)
      (fields
        (field (name INDUCTANCE) 4.7uH)
        (field (name PARTNO) 74404032047)
        (field (name RATE) 1.2A)
        (field (name TOL) ±20%))
      (libsource (lib FunKey) (part 74404032047) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 59450169)))
  (libparts
    (libpart (lib FunKey) (part 74404032047)
      (fields
        (field (name Reference) L)
        (field (name Value) 74404032047))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part AXP20)
      (fields
        (field (name Reference) U)
        (field (name Value) AXP20))
      (pins
        (pin (num 1) (name SDA) (type openCol))
        (pin (num 2) (name SCK) (type input))
        (pin (num 3) (name GPIO3) (type BiDi))
        (pin (num 4) (name N_OE) (type input))
        (pin (num 5) (name GPIO2) (type BiDi))
        (pin (num 6) (name N_VBUSEN) (type input))
        (pin (num 7) (name VIN2) (type power_in))
        (pin (num 8) (name LX2) (type passive))
        (pin (num 9) (name PGND2) (type power_in))
        (pin (num 10) (name DCDC2) (type passive))
        (pin (num 11) (name LDO4) (type power_out))
        (pin (num 12) (name LDO2) (type power_out))
        (pin (num 13) (name LDO24IN) (type power_in))
        (pin (num 14) (name VIN3) (type power_in))
        (pin (num 15) (name LX3) (type passive))
        (pin (num 16) (name PGND3) (type power_in))
        (pin (num 17) (name DCDC3) (type passive))
        (pin (num 18) (name GPIO1) (type BiDi))
        (pin (num 19) (name GPIO0) (type BiDi))
        (pin (num 20) (name EXTEN) (type output))
        (pin (num 21) (name APS) (type power_in))
        (pin (num 22) (name AGND) (type power_in))
        (pin (num 23) (name BIAS) (type passive))
        (pin (num 24) (name VREF) (type passive))
        (pin (num 25) (name PWROK) (type output))
        (pin (num 26) (name VINT) (type power_out))
        (pin (num 27) (name LDO1SET) (type passive))
        (pin (num 28) (name LDO1) (type power_out))
        (pin (num 29) (name DC3SET) (type passive))
        (pin (num 30) (name BACKUP) (type passive))
        (pin (num 31) (name VBUS) (type power_in))
        (pin (num 32) (name ACIN@1) (type power_in))
        (pin (num 33) (name ACIN@2) (type power_in))
        (pin (num 34) (name IPSOUT@1) (type power_out))
        (pin (num 35) (name IPSOUT@2) (type power_in))
        (pin (num 36) (name CHGLED) (type output))
        (pin (num 37) (name TS) (type passive))
        (pin (num 38) (name BAT@1) (type power_in))
        (pin (num 39) (name BAT@2) (type power_in))
        (pin (num 40) (name LDO3IN) (type power_in))
        (pin (num 41) (name LDO3) (type power_out))
        (pin (num 42) (name BATSENSE) (type passive))
        (pin (num 43) (name CHSENSE) (type passive))
        (pin (num 44) (name VIN1) (type power_in))
        (pin (num 45) (name LX1) (type passive))
        (pin (num 46) (name PGND1) (type power_in))
        (pin (num 47) (name PWRON) (type input))
        (pin (num 48) (name IRQ/WAKEUP) (type openCol))
        (pin (num GND$1) (name EP) (type power_in))
        (pin (num GND$2) (name EP) (type power_in))
        (pin (num GND$3) (name EP) (type power_in))
        (pin (num GND$4) (name EP) (type power_in))
        (pin (num GND$5) (name EP) (type power_in))
        (pin (num GND$6) (name EP) (type power_in))
        (pin (num GND$7) (name EP) (type power_in))
        (pin (num GND$8) (name EP) (type power_in))
        (pin (num GND$9) (name EP) (type power_in))))
    (libpart (lib FunKey) (part CAP_0402)
      (fields
        (field (name Reference) C)
        (field (name Value) CAP_0402))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part CAP_1206)
      (fields
        (field (name Reference) C)
        (field (name Value) CAP_1206))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part CDM-10008)
      (fields
        (field (name Reference) SP)
        (field (name Value) CDM-10008)))
    (libpart (lib FunKey) (part CRYSTAL_2SH)
      (fields
        (field (name Reference) Y)
        (field (name Value) CRYSTAL_2SH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib FunKey) (part DF37NB-24DS-0.4V)
      (fields
        (field (name Reference) J)
        (field (name Value) DF37NB-24DS-0.4V))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name 14) (type passive))
        (pin (num 15) (name 15) (type passive))
        (pin (num 16) (name 16) (type passive))
        (pin (num 17) (name 17) (type passive))
        (pin (num 18) (name 18) (type passive))
        (pin (num 19) (name 19) (type passive))
        (pin (num 20) (name 20) (type passive))
        (pin (num 21) (name 21) (type passive))
        (pin (num 22) (name 22) (type passive))
        (pin (num 23) (name 23) (type passive))
        (pin (num 24) (name 24) (type passive))
        (pin (num F$1) (name F@1) (type passive))
        (pin (num F$2) (name F@2) (type passive))))
    (libpart (lib FunKey) (part ESD0402)
      (fields
        (field (name Reference) D)
        (field (name Value) ESD0402))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part EVP-AE)
      (fields
        (field (name Reference) S)
        (field (name Value) EVP-AE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 1') (name A') (type passive))
        (pin (num 2) (name B') (type passive))))
    (libpart (lib FunKey) (part EVP-BB)
      (fields
        (field (name Reference) S)
        (field (name Value) EVP-BB))
      (pins
        (pin (num A) (name A) (type passive))
        (pin (num A') (name A') (type passive))
        (pin (num B) (name B) (type passive))
        (pin (num B') (name B') (type passive))))
    (libpart (lib FunKey) (part FB_0603)
      (fields
        (field (name Reference) L)
        (field (name Value) FB_0603))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part FB_1206)
      (fields
        (field (name Reference) L)
        (field (name Value) FB_1206))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part FC-12M)
      (fields
        (field (name Reference) Y)
        (field (name Value) FC-12M))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part FIDUCIAL)
      (fields
        (field (name Reference) F)
        (field (name Value) FIDUCIAL)))
    (libpart (lib FunKey) (part IRLML2244TRPBF)
      (fields
        (field (name Reference) Q)
        (field (name Value) IRLML2244TRPBF))
      (pins
        (pin (num 1) (name G) (type passive))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib FunKey) (part L1008-)
      (fields
        (field (name Reference) L)
        (field (name Value) L1008-))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part LED_0402)
      (fields
        (field (name Reference) D)
        (field (name Value) LED_0402))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib FunKey) (part MH3-1-0.05)
      (fields
        (field (name Reference) J)
        (field (name Value) MH3-1-0.05))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib FunKey) (part MK24--?3)
      (fields
        (field (name Reference) S)
        (field (name Value) MK24--?3))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib FunKey) (part PAM8301AAF)
      (fields
        (field (name Reference) U)
        (field (name Value) PAM8301AAF))
      (pins
        (pin (num 1) (name OUT-) (type passive))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name IN) (type passive))
        (pin (num 4) (name ~SD) (type input))
        (pin (num 5) (name VDD) (type power_in))
        (pin (num 6) (name OUT+) (type passive))))
    (libpart (lib FunKey) (part PCAL6416A?,128HF)
      (fields
        (field (name Reference) U)
        (field (name Value) PCAL6416A?,128HF))
      (pins
        (pin (num 1) (name P0_0) (type BiDi))
        (pin (num 2) (name P0_1) (type BiDi))
        (pin (num 3) (name P0_2) (type BiDi))
        (pin (num 4) (name P0_3) (type BiDi))
        (pin (num 5) (name P0_4) (type BiDi))
        (pin (num 6) (name P0_5) (type BiDi))
        (pin (num 7) (name P0_6) (type BiDi))
        (pin (num 8) (name P0_7) (type BiDi))
        (pin (num 9) (name VSS) (type power_in))
        (pin (num 10) (name P1_0) (type BiDi))
        (pin (num 11) (name P1_1) (type BiDi))
        (pin (num 12) (name P1_2) (type BiDi))
        (pin (num 13) (name P1_3) (type BiDi))
        (pin (num 14) (name P1_4) (type BiDi))
        (pin (num 15) (name P1_5) (type BiDi))
        (pin (num 16) (name P1_6) (type BiDi))
        (pin (num 17) (name P1_7) (type BiDi))
        (pin (num 18) (name ADDR) (type input))
        (pin (num 19) (name SCL) (type input))
        (pin (num 20) (name SDA) (type BiDi))
        (pin (num 21) (name VDDP) (type power_in))
        (pin (num 22) (name ~INT) (type openCol))
        (pin (num 23) (name VDD) (type power_in))
        (pin (num 24) (name ~RESET) (type input))
        (pin (num 25) (name PAD) (type power_in))))
    (libpart (lib FunKey) (part PRTR5V0U2X,215)
      (fields
        (field (name Reference) D)
        (field (name Value) PRTR5V0U2X,215))
      (pins
        (pin (num 1) (name P$1) (type passive))
        (pin (num 2) (name P$2) (type passive))
        (pin (num 3) (name P$3) (type passive))
        (pin (num 4) (name P$4) (type passive))))
    (libpart (lib FunKey) (part RES_0402)
      (fields
        (field (name Reference) R)
        (field (name Value) RES_0402))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part RES_0603)
      (fields
        (field (name Reference) R)
        (field (name Value) RES_0603))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib FunKey) (part SM02B-SRSS-TB)
      (fields
        (field (name Reference) J)
        (field (name Value) SM02B-SRSS-TB))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num G$1) (name G@1) (type power_in))
        (pin (num G$2) (name G@2) (type power_in))))
    (libpart (lib FunKey) (part SY8088AAC)
      (fields
        (field (name Reference) U)
        (field (name Value) SY8088AAC))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name SW) (type passive))
        (pin (num 4) (name VIN) (type power_in))
        (pin (num 5) (name FB) (type passive))))
    (libpart (lib FunKey) (part TEST_PAD)
      (fields
        (field (name Reference) TP)
        (field (name Value) TEST_PAD))
      (pins
        (pin (num 1) (name PP) (type passive))))
    (libpart (lib FunKey) (part TF-110)
      (fields
        (field (name Reference) J)
        (field (name Value) TF-110))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name CD/DAT3) (type BiDi))
        (pin (num 3) (name CMD) (type input))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type BiDi))
        (pin (num 8) (name DAT1) (type BiDi))
        (pin (num 9) (name DET) (type passive))
        (pin (num 10) (name POL) (type passive))
        (pin (num G$1) (name GND@1) (type power_in))
        (pin (num G$2) (name GND@2) (type power_in))
        (pin (num G$3) (name GND@3) (type power_in))
        (pin (num G$4) (name GND@4) (type power_in))
        (pin (num G$5) (name GND@5) (type power_in))
        (pin (num G$6) (name GND@6) (type power_in))
        (pin (num G$7) (name GND@7) (type power_in))
        (pin (num G$8) (name GND@8) (type power_in))))
    (libpart (lib FunKey) (part U02-BFD3111B0-009)
      (fields
        (field (name Reference) J)
        (field (name Value) U02-BFD3111B0-009))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num S$1) (name M0) (type passive))
        (pin (num S$2) (name M1) (type passive))
        (pin (num S$3) (name M2) (type passive))
        (pin (num S$4) (name M3) (type passive))))
    (libpart (lib FunKey) (part V3S)
      (fields
        (field (name Reference) U)
        (field (name Value) V3S))
      (pins
        (pin (num 1) (name PG4/SDC1_D2/PG_EINT4) (type BiDi))
        (pin (num 2) (name PG3/SDC1_D1/PG_EINT3) (type BiDi))
        (pin (num 3) (name PG2/SDC1_D0/PG_EINT2) (type BiDi))
        (pin (num 4) (name PG1/SDC1_CMD/PG_EINT1) (type BiDi))
        (pin (num 5) (name PG0/SDC1_CLK/PG_EINT0) (type BiDi))
        (pin (num 6) (name PE24/LCD_D23) (type BiDi))
        (pin (num 7) (name PE23/LCD_D22) (type BiDi))
        (pin (num 8) (name PE22/CSI_SDA/TWI1_SDA/UART1_RX) (type BiDi))
        (pin (num 9) (name PE21/CSI_SCK/TWI1_SCK/UART1_TX) (type BiDi))
        (pin (num 10) (name PE20/CSI_FIELD/CSI_MIPI_MCLK) (type BiDi))
        (pin (num 11) (name PE19/CSI_D15/LCD_D21) (type BiDi))
        (pin (num 12) (name VCC-PE0) (type power_in))
        (pin (num 13) (name PE18/CSI_D14/LCD_D20) (type BiDi))
        (pin (num 14) (name PE17/CSI_D13/LCD_D19) (type BiDi))
        (pin (num 15) (name PE16/CSI_D12/LCD_D18) (type BiDi))
        (pin (num 16) (name PE15/CSI_D11/LCD_D15) (type BiDi))
        (pin (num 17) (name PE14/CSI_D10/LCD_D14) (type BiDi))
        (pin (num 18) (name PE13/CSI_D9/LCD_D13) (type BiDi))
        (pin (num 19) (name VDD-SYS3) (type power_in))
        (pin (num 20) (name VDD-CPU3) (type power_in))
        (pin (num 21) (name VDD-CPU2) (type power_in))
        (pin (num 22) (name PE12/CSI_D8/LCD_D12) (type BiDi))
        (pin (num 23) (name PE11/CSI_D7/LCD_D11) (type BiDi))
        (pin (num 24) (name PE10/CSI_D6/LCD_D10) (type BiDi))
        (pin (num 25) (name VDD-CPU1) (type power_in))
        (pin (num 26) (name VDD-CPU0) (type power_in))
        (pin (num 27) (name PE9/CSI_D5/LCD_D7) (type BiDi))
        (pin (num 28) (name PE8/CSI_D4/LCD_D6) (type BiDi))
        (pin (num 29) (name VCC-PE1) (type power_in))
        (pin (num 30) (name PE7/CSI_D3/LCD_D5) (type BiDi))
        (pin (num 31) (name PE6/CSI_D2/LCD_D4) (type BiDi))
        (pin (num 32) (name PE5/CSI_D1/LCD_D3) (type BiDi))
        (pin (num 33) (name PE4/CSI_D0/LCD_D2) (type passive))
        (pin (num 34) (name PE3/CSI_VSYNC/LCD_VSYNC) (type BiDi))
        (pin (num 35) (name PE2/CSI_HSYNC/LCD_HSYNC) (type BiDi))
        (pin (num 36) (name PE1/CSI_MCLK/LCD_DE) (type BiDi))
        (pin (num 37) (name PE0/CSI_PCLK-/LCD_CLK) (type BiDi))
        (pin (num 38) (name VDD-CPU4) (type power_in))
        (pin (num 39) (name PB0/UART2_TX/PB_EINT0) (type BiDi))
        (pin (num 40) (name PB1/UART2_RX/PB_EINT1) (type BiDi))
        (pin (num 41) (name PB2/UART2_RTS/PB_EINT2) (type BiDi))
        (pin (num 42) (name PB3/UART2_CTS/PB_EINT3) (type BiDi))
        (pin (num 43) (name PB4/PWM0/PB_EINT4) (type BiDi))
        (pin (num 44) (name PB5/PWM1/PB_EINT5) (type BiDi))
        (pin (num 45) (name PB6/TWI0_SCK/PB_EINT6) (type BiDi))
        (pin (num 46) (name PB7/TWI0_SDA/PB_EINT7) (type BiDi))
        (pin (num 47) (name VDD-CPU5) (type power_in))
        (pin (num 48) (name PB8/TWI1_SCK/UART0_TX/PB_EINT8) (type BiDi))
        (pin (num 49) (name PB9/TWI1_SDA/UART0_RX/PB_EINT9) (type BiDi))
        (pin (num 50) (name VCC-IO3) (type power_in))
        (pin (num 51) (name VDD-CPU6) (type power_in))
        (pin (num 52) (name PC0/SDC2_CLK/SPI_MISO) (type BiDi))
        (pin (num 53) (name PC1/SDC2_CMD/SPI_CLK) (type BiDi))
        (pin (num 54) (name PC2/SDC2_RST/SPI_CS) (type BiDi))
        (pin (num 55) (name PC3/SDC2_D0/SPI_MOSI) (type BiDi))
        (pin (num 56) (name VDD-CPU7) (type power_in))
        (pin (num 57) (name VCC-IO2) (type power_in))
        (pin (num 58) (name VDD-SYS4) (type power_in))
        (pin (num 59) (name VCC-DRAM8) (type power_in))
        (pin (num 60) (name VCC-DRAM9) (type power_in))
        (pin (num 61) (name VCC-DRAM10) (type power_in))
        (pin (num 62) (name VCC-DRAM11) (type power_in))
        (pin (num 63) (name SVREF1) (type passive))
        (pin (num 64) (name VDD-SYS5) (type power_in))
        (pin (num 65) (name VCC-DRAM0) (type power_in))
        (pin (num 66) (name VCC-DRAM1) (type power_in))
        (pin (num 67) (name VCC-DRAM2) (type power_in))
        (pin (num 68) (name VCC-DRAM3) (type power_in))
        (pin (num 69) (name VCC-DRAM4) (type power_in))
        (pin (num 70) (name VCC-DRAM5) (type power_in))
        (pin (num 71) (name SVREF0) (type passive))
        (pin (num 72) (name VCC-DRAM6) (type power_in))
        (pin (num 73) (name SZQ) (type passive))
        (pin (num 74) (name X24MOUT) (type passive))
        (pin (num 75) (name X24MIN) (type passive))
        (pin (num 76) (name VCC-PLL) (type power_in))
        (pin (num 77) (name EPHY-LINK-LED) (type passive))
        (pin (num 78) (name EPHY-SPD-LED) (type passive))
        (pin (num 79) (name VCC-DRAM7) (type power_in))
        (pin (num 80) (name VDD-SYS0) (type power_in))
        (pin (num 81) (name MCSI-D0P) (type input))
        (pin (num 82) (name MCSI-D0N) (type input))
        (pin (num 83) (name MCSI-D1P) (type input))
        (pin (num 84) (name MCSI-D1N) (type input))
        (pin (num 85) (name VCC-MCSI) (type input))
        (pin (num 86) (name MCSI-CKP) (type output))
        (pin (num 87) (name MCSI-CKN) (type output))
        (pin (num 88) (name EPHY-VDD) (type passive))
        (pin (num 89) (name EPHY-RXN) (type passive))
        (pin (num 90) (name EPHY-RXP) (type passive))
        (pin (num 91) (name EPHY-TXN) (type passive))
        (pin (num 92) (name EPHY-TXP) (type passive))
        (pin (num 93) (name EPHY-VCC) (type passive))
        (pin (num 94) (name EPHY-RTX) (type passive))
        (pin (num 95) (name X32KOUT) (type passive))
        (pin (num 96) (name X32KIN) (type passive))
        (pin (num 97) (name RTC-VIO) (type passive))
        (pin (num 98) (name VCC-RTC) (type power_in))
        (pin (num 99) (name RESET) (type input))
        (pin (num 100) (name PF6) (type BiDi))
        (pin (num 101) (name PF5/SDC0_D2/JTAG_CK1) (type BiDi))
        (pin (num 102) (name PF4/SDC0_D3/UART0_RX) (type BiDi))
        (pin (num 103) (name PF3/SDC0_CMD/JTAG_DO1) (type BiDi))
        (pin (num 104) (name VCC-IO0) (type power_in))
        (pin (num 105) (name PF2/SDC0_CLK/UART0_TX) (type BiDi))
        (pin (num 106) (name PF1/SDC0_D0/JTAG_DI1) (type BiDi))
        (pin (num 107) (name PF0/SDC0_D1/JTAG_MS1) (type BiDi))
        (pin (num 108) (name VDD-SYS1) (type power_in))
        (pin (num 109) (name VCC-USB) (type power_in))
        (pin (num 110) (name USB-DM) (type passive))
        (pin (num 111) (name USB-DP) (type passive))
        (pin (num 112) (name LRADC0) (type passive))
        (pin (num 113) (name MICIN1P) (type passive))
        (pin (num 114) (name MICIN1N) (type passive))
        (pin (num 115) (name AVCC) (type power_in))
        (pin (num 116) (name AGND) (type power_in))
        (pin (num 117) (name VRA1) (type power_out))
        (pin (num 118) (name VRA2) (type power_out))
        (pin (num 119) (name HBIAS) (type passive))
        (pin (num 120) (name HPOUTR) (type passive))
        (pin (num 121) (name HPOUTL) (type passive))
        (pin (num 122) (name HPVCCIN) (type power_in))
        (pin (num 123) (name HPVCCBP) (type power_out))
        (pin (num 124) (name HPCOMFB) (type passive))
        (pin (num 125) (name HPCOM) (type passive))
        (pin (num 126) (name VDD-SYS2) (type power_in))
        (pin (num 127) (name VCC-IO1) (type power_in))
        (pin (num 128) (name PG5/SDC1_D3/PG_EINT5) (type BiDi))
        (pin (num GND$1) (name EGND) (type power_in))
        (pin (num GND$2) (name EGND) (type power_in))
        (pin (num GND$3) (name EGND) (type power_in))
        (pin (num GND$4) (name EGND) (type power_in))
        (pin (num GND$5) (name EGND) (type power_in))
        (pin (num GND$6) (name EGND) (type power_in))
        (pin (num GND$7) (name EGND) (type power_in))
        (pin (num GND$8) (name EGND) (type power_in))
        (pin (num GND$9) (name EGND) (type power_in)))))
  (libraries
    (library (logical FunKey)
      (uri FunKey.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref S11) (pin A))
      (node (ref C83) (pin 2))
      (node (ref S6) (pin A))
      (node (ref S5) (pin A'))
      (node (ref S5) (pin A))
      (node (ref S4) (pin A'))
      (node (ref S3) (pin A'))
      (node (ref S3) (pin A))
      (node (ref S11) (pin A'))
      (node (ref S4) (pin A))
      (node (ref J5) (pin G$1))
      (node (ref J5) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref S6) (pin A'))
      (node (ref S2) (pin A'))
      (node (ref S2) (pin A))
      (node (ref D20) (pin 2))
      (node (ref D21) (pin 2))
      (node (ref D22) (pin 2))
      (node (ref D19) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U3) (pin GND$9))
      (node (ref S8) (pin A'))
      (node (ref S9) (pin A'))
      (node (ref S9) (pin A))
      (node (ref D11) (pin 2))
      (node (ref S8) (pin A))
      (node (ref D6) (pin 2))
      (node (ref D9) (pin 2))
      (node (ref D10) (pin 2))
      (node (ref U3) (pin GND$8))
      (node (ref D13) (pin 2))
      (node (ref D14) (pin 2))
      (node (ref C50) (pin 1))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 2))
      (node (ref J3) (pin 12))
      (node (ref U3) (pin 33))
      (node (ref U3) (pin 116))
      (node (ref C55) (pin 1))
      (node (ref C52) (pin 2))
      (node (ref R22) (pin 1))
      (node (ref C67) (pin 2))
      (node (ref C64) (pin 1))
      (node (ref D5) (pin 2))
      (node (ref U3) (pin GND$7))
      (node (ref U3) (pin GND$6))
      (node (ref U3) (pin GND$5))
      (node (ref U3) (pin GND$4))
      (node (ref U3) (pin GND$3))
      (node (ref U3) (pin GND$2))
      (node (ref U3) (pin GND$1))
      (node (ref D8) (pin 2))
      (node (ref S10) (pin A))
      (node (ref C23) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref J4) (pin G$1))
      (node (ref J4) (pin 9))
      (node (ref J4) (pin 6))
      (node (ref J4) (pin G$2))
      (node (ref S7) (pin 1'))
      (node (ref S7) (pin 1))
      (node (ref S12) (pin 2))
      (node (ref D32) (pin 2))
      (node (ref TP25) (pin 1))
      (node (ref J2) (pin 5))
      (node (ref S13) (pin B'))
      (node (ref S13) (pin B))
      (node (ref D29) (pin 2))
      (node (ref D24) (pin 2))
      (node (ref D31) (pin 2))
      (node (ref S1) (pin A'))
      (node (ref S1) (pin A))
      (node (ref U1) (pin 18))
      (node (ref J4) (pin 10))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 25))
      (node (ref J4) (pin G$8))
      (node (ref J4) (pin G$7))
      (node (ref J4) (pin G$6))
      (node (ref J4) (pin G$5))
      (node (ref J4) (pin G$4))
      (node (ref J4) (pin G$3))
      (node (ref D4) (pin 2))
      (node (ref C32) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref C47) (pin 1))
      (node (ref D12) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref D23) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref S10) (pin A'))
      (node (ref C18) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref C62) (pin 2))
      (node (ref C51) (pin 1))
      (node (ref C21) (pin 2))
      (node (ref C82) (pin 1))
      (node (ref C76) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref C45) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C49) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref C68) (pin 2))
      (node (ref U5) (pin 46))
      (node (ref D16) (pin 2))
      (node (ref D15) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C44) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref U5) (pin GND$1))
      (node (ref U5) (pin GND$2))
      (node (ref C46) (pin 1))
      (node (ref U5) (pin GND$3))
      (node (ref C9) (pin 1))
      (node (ref C65) (pin 1))
      (node (ref C20) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C37) (pin 1))
      (node (ref R23) (pin 1))
      (node (ref C73) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref C77) (pin 1))
      (node (ref C61) (pin 1))
      (node (ref C48) (pin 1))
      (node (ref U5) (pin 9))
      (node (ref C39) (pin 1))
      (node (ref C70) (pin 2))
      (node (ref C59) (pin 2))
      (node (ref C43) (pin 1))
      (node (ref C34) (pin 2))
      (node (ref C30) (pin 1))
      (node (ref C72) (pin 2))
      (node (ref C38) (pin 1))
      (node (ref C69) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref U5) (pin GND$7))
      (node (ref C78) (pin 2))
      (node (ref U5) (pin GND$6))
      (node (ref R24) (pin 2))
      (node (ref U5) (pin GND$9))
      (node (ref U5) (pin GND$8))
      (node (ref C29) (pin 1))
      (node (ref C60) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref C75) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref Y2) (pin 4))
      (node (ref Y2) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U5) (pin 16))
      (node (ref C26) (pin 1))
      (node (ref U5) (pin 22))
      (node (ref U5) (pin 6))
      (node (ref C33) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref D28) (pin 2))
      (node (ref D27) (pin 2))
      (node (ref D26) (pin 2))
      (node (ref D25) (pin 2))
      (node (ref D18) (pin 2))
      (node (ref D17) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref R28) (pin 1))
      (node (ref C66) (pin 2))
      (node (ref C81) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref C74) (pin 2))
      (node (ref C57) (pin 2))
      (node (ref C58) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref U5) (pin GND$5))
      (node (ref U5) (pin GND$4))
      (node (ref R11) (pin 1))
      (node (ref C42) (pin 2)))
    (net (code 2) (name /LRADC0)
      (node (ref C9) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref U3) (pin 112)))
    (net (code 3) (name HPVCCBP)
      (node (ref C57) (pin 1))
      (node (ref U3) (pin 123))
      (node (ref C61) (pin 2)))
    (net (code 4) (name +3V0)
      (node (ref TP17) (pin 1))
      (node (ref U3) (pin 115))
      (node (ref U3) (pin 76))
      (node (ref U5) (pin 12))
      (node (ref C33) (pin 2))
      (node (ref C74) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref C51) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref C77) (pin 2)))
    (net (code 5) (name /EN)
      (node (ref U4) (pin 1))
      (node (ref R19) (pin 1)))
    (net (code 6) (name +1V8)
      (node (ref TP16) (pin 1))
      (node (ref C58) (pin 1))
      (node (ref C80) (pin 2))
      (node (ref C76) (pin 2))
      (node (ref C65) (pin 2))
      (node (ref C66) (pin 1))
      (node (ref C71) (pin 2))
      (node (ref R25) (pin 2))
      (node (ref C73) (pin 2))
      (node (ref L6) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref C62) (pin 1))
      (node (ref U3) (pin 66))
      (node (ref U3) (pin 65))
      (node (ref U3) (pin 62))
      (node (ref U3) (pin 61))
      (node (ref U3) (pin 60))
      (node (ref U3) (pin 59))
      (node (ref U3) (pin 67))
      (node (ref U3) (pin 68))
      (node (ref U3) (pin 69))
      (node (ref U3) (pin 72))
      (node (ref U3) (pin 70))
      (node (ref U3) (pin 79)))
    (net (code 7) (name SVREF)
      (node (ref R25) (pin 1))
      (node (ref U3) (pin 71))
      (node (ref R28) (pin 2))
      (node (ref U3) (pin 63))
      (node (ref C80) (pin 1))
      (node (ref C82) (pin 2)))
    (net (code 8) (name "Net-(D30-Pad2)")
      (node (ref R26) (pin 1))
      (node (ref D30) (pin 2)))
    (net (code 9) (name /VBUS)
      (node (ref C7) (pin 1))
      (node (ref D15) (pin 4))
      (node (ref L2) (pin 1))
      (node (ref J2) (pin 1)))
    (net (code 10) (name /UART0_TX0)
      (node (ref R3) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 11) (name /X)
      (node (ref S9) (pin B'))
      (node (ref U1) (pin 15))
      (node (ref S9) (pin B))
      (node (ref D4) (pin 1)))
    (net (code 12) (name +VIN)
      (node (ref U5) (pin 33))
      (node (ref U5) (pin 32))
      (node (ref C75) (pin 1)))
    (net (code 13) (name /~RESET)
      (node (ref TP1) (pin 1))
      (node (ref U5) (pin 25))
      (node (ref R15) (pin 2))
      (node (ref U3) (pin 99))
      (node (ref U1) (pin 24))
      (node (ref C18) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 14) (name /VINT)
      (node (ref U5) (pin 26))
      (node (ref U5) (pin 27))
      (node (ref C67) (pin 1)))
    (net (code 15) (name "Net-(U5-Pad3)")
      (node (ref U5) (pin 3)))
    (net (code 16) (name "Net-(U5-Pad30)")
      (node (ref U5) (pin 30)))
    (net (code 17) (name /LDO4)
      (node (ref U5) (pin 11))
      (node (ref C38) (pin 2)))
    (net (code 18) (name "Net-(U5-Pad18)")
      (node (ref U5) (pin 18)))
    (net (code 19) (name "Net-(U5-Pad19)")
      (node (ref U5) (pin 19)))
    (net (code 20) (name "Net-(U5-Pad20)")
      (node (ref U5) (pin 20)))
    (net (code 21) (name /B)
      (node (ref U1) (pin 14))
      (node (ref D2) (pin 1))
      (node (ref S11) (pin B'))
      (node (ref S11) (pin B)))
    (net (code 22) (name /U)
      (node (ref U1) (pin 4))
      (node (ref S3) (pin B'))
      (node (ref S3) (pin B))
      (node (ref D6) (pin 1)))
    (net (code 23) (name /FUN)
      (node (ref S2) (pin B))
      (node (ref D5) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref S2) (pin B')))
    (net (code 24) (name /START)
      (node (ref U1) (pin 7))
      (node (ref D8) (pin 1))
      (node (ref S1) (pin B'))
      (node (ref S1) (pin B)))
    (net (code 25) (name /Y)
      (node (ref U1) (pin 13))
      (node (ref D7) (pin 1))
      (node (ref S8) (pin B'))
      (node (ref S8) (pin B)))
    (net (code 26) (name /A)
      (node (ref S10) (pin B'))
      (node (ref S10) (pin B))
      (node (ref U1) (pin 16))
      (node (ref D3) (pin 1)))
    (net (code 27) (name /SW)
      (node (ref U4) (pin 3))
      (node (ref L6) (pin 1)))
    (net (code 28) (name +VOUT)
      (node (ref U5) (pin 21))
      (node (ref U5) (pin 35))
      (node (ref U5) (pin 34))
      (node (ref U5) (pin 14))
      (node (ref C59) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref R26) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref S14) (pin 1))
      (node (ref U4) (pin 4))
      (node (ref U5) (pin 7))
      (node (ref C37) (pin 2))
      (node (ref U5) (pin 44))
      (node (ref C78) (pin 1))
      (node (ref TP23) (pin 1))
      (node (ref C55) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C52) (pin 1))
      (node (ref U5) (pin 29)))
    (net (code 29) (name /LDO3)
      (node (ref C63) (pin 1))
      (node (ref U5) (pin 41)))
    (net (code 30) (name +VBAT)
      (node (ref R21) (pin 1))
      (node (ref TP20) (pin 1))
      (node (ref C60) (pin 1))
      (node (ref U5) (pin 39))
      (node (ref U5) (pin 38))
      (node (ref J5) (pin 1))
      (node (ref C56) (pin 2))
      (node (ref U5) (pin 42)))
    (net (code 31) (name /LX1)
      (node (ref L5) (pin 1))
      (node (ref U5) (pin 45)))
    (net (code 32) (name /PWRON)
      (node (ref U5) (pin 47))
      (node (ref R18) (pin 1))
      (node (ref C42) (pin 1)))
    (net (code 33) (name "Net-(U5-Pad5)")
      (node (ref U5) (pin 5)))
    (net (code 34) (name /POWER)
      (node (ref TP22) (pin 1))
      (node (ref S13) (pin A))
      (node (ref D29) (pin 1))
      (node (ref S13) (pin A'))
      (node (ref R18) (pin 2)))
    (net (code 35) (name "Net-(U3-Pad24)")
      (node (ref U3) (pin 24)))
    (net (code 36) (name "Net-(U3-Pad16)")
      (node (ref U3) (pin 16)))
    (net (code 37) (name "Net-(U3-Pad17)")
      (node (ref U3) (pin 17)))
    (net (code 38) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 39) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 40) (name "Net-(U3-Pad22)")
      (node (ref U3) (pin 22)))
    (net (code 41) (name "Net-(U3-Pad23)")
      (node (ref U3) (pin 23)))
    (net (code 42) (name "Net-(U3-Pad15)")
      (node (ref U3) (pin 15)))
    (net (code 43) (name "Net-(U3-Pad27)")
      (node (ref U3) (pin 27)))
    (net (code 44) (name "Net-(U3-Pad28)")
      (node (ref U3) (pin 28)))
    (net (code 45) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 46) (name "Net-(U3-Pad30)")
      (node (ref U3) (pin 30)))
    (net (code 47) (name "Net-(U3-Pad31)")
      (node (ref U3) (pin 31)))
    (net (code 48) (name "Net-(U3-Pad32)")
      (node (ref U3) (pin 32)))
    (net (code 49) (name "Net-(U3-Pad114)")
      (node (ref U3) (pin 114)))
    (net (code 50) (name "Net-(U3-Pad119)")
      (node (ref U3) (pin 119)))
    (net (code 51) (name "Net-(U3-Pad121)")
      (node (ref U3) (pin 121)))
    (net (code 52) (name "Net-(U3-Pad128)")
      (node (ref U3) (pin 128)))
    (net (code 53) (name "Net-(U3-Pad13)")
      (node (ref U3) (pin 13)))
    (net (code 54) (name "Net-(U3-Pad14)")
      (node (ref U3) (pin 14)))
    (net (code 55) (name "Net-(U3-Pad6)")
      (node (ref U3) (pin 6)))
    (net (code 56) (name "Net-(U3-Pad34)")
      (node (ref U3) (pin 34)))
    (net (code 57) (name "Net-(U3-Pad35)")
      (node (ref U3) (pin 35)))
    (net (code 58) (name "Net-(U3-Pad36)")
      (node (ref U3) (pin 36)))
    (net (code 59) (name "Net-(U3-Pad37)")
      (node (ref U3) (pin 37)))
    (net (code 60) (name "Net-(U3-Pad39)")
      (node (ref U3) (pin 39)))
    (net (code 61) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 62) (name /TE)
      (node (ref U3) (pin 40))
      (node (ref TP34) (pin 1))
      (node (ref J3) (pin 9))
      (node (ref D32) (pin 1)))
    (net (code 63) (name /LCD_RESET)
      (node (ref TP18) (pin 1))
      (node (ref D21) (pin 1))
      (node (ref J3) (pin 11))
      (node (ref U3) (pin 41))
      (node (ref R29) (pin 2)))
    (net (code 64) (name "Net-(U3-Pad113)")
      (node (ref U3) (pin 113)))
    (net (code 65) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 66) (name "Net-(J3-Pad22)")
      (node (ref J3) (pin 22)))
    (net (code 67) (name "Net-(J3-PadF$1)")
      (node (ref J3) (pin F$1)))
    (net (code 68) (name "Net-(J3-PadF$2)")
      (node (ref J3) (pin F$2)))
    (net (code 69) (name "Net-(J3-Pad24)")
      (node (ref J3) (pin 24)))
    (net (code 70) (name "Net-(J3-Pad23)")
      (node (ref J3) (pin 23)))
    (net (code 71) (name "Net-(J3-Pad21)")
      (node (ref J3) (pin 21)))
    (net (code 72) (name "Net-(J3-Pad20)")
      (node (ref J3) (pin 20)))
    (net (code 73) (name "Net-(J3-Pad18)")
      (node (ref J3) (pin 18)))
    (net (code 74) (name "Net-(J3-Pad19)")
      (node (ref J3) (pin 19)))
    (net (code 75) (name "Net-(J3-Pad17)")
      (node (ref J3) (pin 17)))
    (net (code 76) (name "Net-(J3-Pad16)")
      (node (ref J3) (pin 16)))
    (net (code 77) (name "Net-(J3-Pad15)")
      (node (ref J3) (pin 15)))
    (net (code 78) (name "Net-(J3-Pad14)")
      (node (ref J3) (pin 14)))
    (net (code 79) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13)))
    (net (code 80) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 81) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 10)))
    (net (code 82) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 83) (name +3V3)
      (node (ref R1) (pin 2))
      (node (ref U3) (pin 29))
      (node (ref C20) (pin 1))
      (node (ref C45) (pin 2))
      (node (ref U3) (pin 93))
      (node (ref C41) (pin 2))
      (node (ref R9) (pin 1))
      (node (ref U3) (pin 127))
      (node (ref U3) (pin 12))
      (node (ref U3) (pin 122))
      (node (ref J3) (pin 5))
      (node (ref C17) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref J3) (pin 3))
      (node (ref U3) (pin 104))
      (node (ref U3) (pin 109))
      (node (ref U3) (pin 57))
      (node (ref C25) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref U3) (pin 50))
      (node (ref C2) (pin 2))
      (node (ref U5) (pin 13))
      (node (ref U5) (pin 17))
      (node (ref TP14) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref R13) (pin 2))
      (node (ref C43) (pin 2))
      (node (ref C47) (pin 2))
      (node (ref U3) (pin 85))
      (node (ref C32) (pin 2))
      (node (ref C69) (pin 1))
      (node (ref C28) (pin 2))
      (node (ref C34) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U5) (pin 40))
      (node (ref U1) (pin 21))
      (node (ref C39) (pin 2))
      (node (ref L4) (pin 1))
      (node (ref U1) (pin 23)))
    (net (code 84) (name VRA1)
      (node (ref U3) (pin 117))
      (node (ref C81) (pin 1)))
    (net (code 85) (name VRA2)
      (node (ref U3) (pin 118))
      (node (ref C79) (pin 1))
      (node (ref R27) (pin 2)))
    (net (code 86) (name RTC-VIO)
      (node (ref C68) (pin 1))
      (node (ref U3) (pin 97)))
    (net (code 87) (name HPCOM)
      (node (ref U3) (pin 124))
      (node (ref C54) (pin 1))
      (node (ref U3) (pin 125)))
    (net (code 88) (name +1V25)
      (node (ref L3) (pin 2))
      (node (ref C46) (pin 2))
      (node (ref C48) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref TP13) (pin 1))
      (node (ref U3) (pin 80))
      (node (ref J5) (pin G$2))
      (node (ref U3) (pin 108))
      (node (ref C50) (pin 2))
      (node (ref U5) (pin 10))
      (node (ref C44) (pin 2))
      (node (ref U3) (pin 19))
      (node (ref U3) (pin 88))
      (node (ref U3) (pin 21))
      (node (ref U3) (pin 25))
      (node (ref C21) (pin 1))
      (node (ref U3) (pin 20))
      (node (ref U3) (pin 26))
      (node (ref U3) (pin 126))
      (node (ref C40) (pin 1))
      (node (ref C26) (pin 2))
      (node (ref C35) (pin 1))
      (node (ref U3) (pin 64))
      (node (ref U3) (pin 47))
      (node (ref C16) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref U3) (pin 58))
      (node (ref C29) (pin 2))
      (node (ref U3) (pin 56))
      (node (ref U3) (pin 38))
      (node (ref U3) (pin 51))
      (node (ref C27) (pin 2))
      (node (ref C31) (pin 1)))
    (net (code 89) (name "Net-(U3-Pad91)")
      (node (ref U3) (pin 91)))
    (net (code 90) (name "Net-(U3-Pad77)")
      (node (ref U3) (pin 77)))
    (net (code 91) (name "Net-(U3-Pad81)")
      (node (ref U3) (pin 81)))
    (net (code 92) (name "Net-(U3-Pad82)")
      (node (ref U3) (pin 82)))
    (net (code 93) (name "Net-(U3-Pad83)")
      (node (ref U3) (pin 83)))
    (net (code 94) (name "Net-(U3-Pad84)")
      (node (ref U3) (pin 84)))
    (net (code 95) (name "Net-(U3-Pad86)")
      (node (ref U3) (pin 86)))
    (net (code 96) (name "Net-(U3-Pad87)")
      (node (ref U3) (pin 87)))
    (net (code 97) (name "Net-(U3-Pad89)")
      (node (ref U3) (pin 89)))
    (net (code 98) (name "Net-(U3-Pad90)")
      (node (ref U3) (pin 90)))
    (net (code 99) (name "Net-(U3-Pad92)")
      (node (ref U3) (pin 92)))
    (net (code 100) (name "Net-(U3-Pad94)")
      (node (ref U3) (pin 94)))
    (net (code 101) (name "Net-(U3-Pad78)")
      (node (ref U3) (pin 78)))
    (net (code 102) (name "Net-(U3-Pad9)")
      (node (ref U3) (pin 9)))
    (net (code 103) (name +3V3_AO)
      (node (ref C72) (pin 1))
      (node (ref TP15) (pin 1))
      (node (ref U3) (pin 98))
      (node (ref R15) (pin 1))
      (node (ref U5) (pin 28))
      (node (ref C49) (pin 2)))
    (net (code 104) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 105) (name /SZQ)
      (node (ref R11) (pin 2))
      (node (ref U3) (pin 73)))
    (net (code 106) (name /X24MOUT)
      (node (ref Y2) (pin 1))
      (node (ref U3) (pin 74))
      (node (ref C13) (pin 2)))
    (net (code 107) (name /X24MIN)
      (node (ref U3) (pin 75))
      (node (ref C12) (pin 2))
      (node (ref Y2) (pin 3)))
    (net (code 108) (name "Net-(U3-Pad8)")
      (node (ref U3) (pin 8)))
    (net (code 109) (name /IN)
      (node (ref U2) (pin 3))
      (node (ref TP12) (pin 1))
      (node (ref C3) (pin 2)))
    (net (code 110) (name PE)
      (node (ref J2) (pin S$3))
      (node (ref J2) (pin S$2))
      (node (ref J2) (pin S$1))
      (node (ref J2) (pin S$4))
      (node (ref C6) (pin 1)))
    (net (code 111) (name "Net-(S12-Pad1')")
      (node (ref S12) (pin 1')))
    (net (code 112) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 113) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 114) (name /R)
      (node (ref S6) (pin B'))
      (node (ref S6) (pin B))
      (node (ref D11) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 115) (name /D)
      (node (ref S5) (pin B))
      (node (ref D10) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref S5) (pin B')))
    (net (code 116) (name +VUSB)
      (node (ref TP19) (pin 1))
      (node (ref C70) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref U5) (pin 31))
      (node (ref C8) (pin 2))
      (node (ref L2) (pin 2)))
    (net (code 117) (name /LEDA)
      (node (ref Q1) (pin 3))
      (node (ref D22) (pin 1))
      (node (ref TP24) (pin 1))
      (node (ref J3) (pin 1)))
    (net (code 118) (name /TWI0_SCK)
      (node (ref TP4) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U1) (pin 19))
      (node (ref U5) (pin 2))
      (node (ref U3) (pin 45)))
    (net (code 119) (name /LX2)
      (node (ref U5) (pin 8))
      (node (ref L3) (pin 1)))
    (net (code 120) (name /LX3)
      (node (ref U5) (pin 15))
      (node (ref L4) (pin 2)))
    (net (code 121) (name /BIAS)
      (node (ref R22) (pin 2))
      (node (ref U5) (pin 23)))
    (net (code 122) (name /VREF)
      (node (ref C64) (pin 2))
      (node (ref U5) (pin 24)))
    (net (code 123) (name /~CHGLED)
      (node (ref TP21) (pin 1))
      (node (ref U5) (pin 36))
      (node (ref D31) (pin 1))
      (node (ref D30) (pin 1)))
    (net (code 124) (name /~PMU_IRQ)
      (node (ref R13) (pin 1))
      (node (ref U3) (pin 44))
      (node (ref TP2) (pin 1))
      (node (ref U5) (pin 48)))
    (net (code 125) (name /N_OE)
      (node (ref U1) (pin 12))
      (node (ref U5) (pin 4))
      (node (ref C83) (pin 1))
      (node (ref TP9) (pin 1))
      (node (ref R17) (pin 2))
      (node (ref S14) (pin 2)))
    (net (code 126) (name /TS)
      (node (ref U5) (pin 37))
      (node (ref R24) (pin 1)))
    (net (code 127) (name /UART0_TX)
      (node (ref U3) (pin 48))
      (node (ref R3) (pin 1)))
    (net (code 128) (name /UART0_RX)
      (node (ref J1) (pin 3))
      (node (ref U3) (pin 49)))
    (net (code 129) (name /~SPI_CS)
      (node (ref J3) (pin 6))
      (node (ref U3) (pin 54))
      (node (ref TP8) (pin 1))
      (node (ref D19) (pin 1)))
    (net (code 130) (name /SPI_CLK)
      (node (ref U3) (pin 53))
      (node (ref D24) (pin 1))
      (node (ref J3) (pin 8))
      (node (ref TP6) (pin 1)))
    (net (code 131) (name /HPOUTR)
      (node (ref U3) (pin 120))
      (node (ref C3) (pin 1)))
    (net (code 132) (name /PA_VDD)
      (node (ref L1) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 133) (name /TWI0_SDA)
      (node (ref U3) (pin 46))
      (node (ref R16) (pin 1))
      (node (ref TP3) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref U1) (pin 20)))
    (net (code 134) (name /SPI_MOSI)
      (node (ref U3) (pin 55))
      (node (ref D20) (pin 1))
      (node (ref TP7) (pin 1))
      (node (ref J3) (pin 7)))
    (net (code 135) (name /SDC0_CMD)
      (node (ref D26) (pin 1))
      (node (ref U3) (pin 103))
      (node (ref TP31) (pin 1))
      (node (ref J4) (pin 3))
      (node (ref R10) (pin 2)))
    (net (code 136) (name /SDC0_CLK)
      (node (ref D18) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref TP30) (pin 1))
      (node (ref J4) (pin 5)))
    (net (code 137) (name /SDC0_D2)
      (node (ref J4) (pin 1))
      (node (ref U3) (pin 101))
      (node (ref D28) (pin 1))
      (node (ref TP33) (pin 1)))
    (net (code 138) (name /SDC0_D3)
      (node (ref U3) (pin 102))
      (node (ref J4) (pin 2))
      (node (ref TP32) (pin 1))
      (node (ref D27) (pin 1)))
    (net (code 139) (name /USB_P)
      (node (ref J2) (pin 3))
      (node (ref U3) (pin 111))
      (node (ref TP27) (pin 1))
      (node (ref D15) (pin 2)))
    (net (code 140) (name /USB_N)
      (node (ref J2) (pin 2))
      (node (ref D15) (pin 3))
      (node (ref U3) (pin 110))
      (node (ref TP26) (pin 1)))
    (net (code 141) (name /SDC0_D0)
      (node (ref U3) (pin 106))
      (node (ref J4) (pin 7))
      (node (ref TP29) (pin 1))
      (node (ref D17) (pin 1)))
    (net (code 142) (name /SDC0_D1)
      (node (ref D16) (pin 1))
      (node (ref TP28) (pin 1))
      (node (ref U3) (pin 107))
      (node (ref J4) (pin 8)))
    (net (code 143) (name /USB_ID)
      (node (ref J2) (pin 4))
      (node (ref R4) (pin 1)))
    (net (code 144) (name /SPK+)
      (node (ref D13) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 145) (name /SPK-)
      (node (ref U2) (pin 1))
      (node (ref D14) (pin 1)))
    (net (code 146) (name /RR)
      (node (ref S7) (pin 2))
      (node (ref U1) (pin 17))
      (node (ref D12) (pin 1)))
    (net (code 147) (name /~KEY_IRQ)
      (node (ref U3) (pin 42))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 22))
      (node (ref TP10) (pin 1)))
    (net (code 148) (name /L)
      (node (ref D9) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref S4) (pin B))
      (node (ref S4) (pin B')))
    (net (code 149) (name /RL)
      (node (ref U1) (pin 3))
      (node (ref S12) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 150) (name /X32KIN)
      (node (ref C14) (pin 2))
      (node (ref Y1) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 96)))
    (net (code 151) (name /X32KOUT)
      (node (ref R12) (pin 1))
      (node (ref U3) (pin 95))
      (node (ref Y1) (pin 1))
      (node (ref C15) (pin 2)))
    (net (code 152) (name /SDC0_CLK0)
      (node (ref U3) (pin 105))
      (node (ref R8) (pin 2)))
    (net (code 153) (name /RS)
      (node (ref TP5) (pin 1))
      (node (ref D23) (pin 1))
      (node (ref J3) (pin 10))
      (node (ref U3) (pin 52)))
    (net (code 154) (name /PWM0)
      (node (ref R5) (pin 1))
      (node (ref U3) (pin 43)))
    (net (code 155) (name /PWM)
      (node (ref R5) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 156) (name /TF-VDD)
      (node (ref J4) (pin 4))
      (node (ref D25) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 157) (name /~PA_SHDN)
      (node (ref TP11) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U3) (pin 100))
      (node (ref U2) (pin 4)))
    (net (code 158) (name /CHSENSE)
      (node (ref C56) (pin 1))
      (node (ref R21) (pin 2))
      (node (ref C53) (pin 1))
      (node (ref L5) (pin 2))
      (node (ref U5) (pin 43)))
    (net (code 159) (name /FB)
      (node (ref R23) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref U4) (pin 5)))))