inotify-tools: fix __NR_inotify_add_watch system call number on _MIPS_SIM_ABI64

The correct value should be the same as defined in
linux/arch/mips/include/uapi/asm/unistd.h

Upstream-Status: Summitted [https://github.com/rvoicilas/inotify-tools/pull/71]

Signed-off-by: Roy Li <rongqing.li@windriver.com>
Signed-off-by: Jackie Huang <jackie.huang@windriver.com>
---
 libinotifytools/src/inotifytools/inotify-nosys.h |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/libinotifytools/src/inotifytools/inotify-nosys.h b/libinotifytools/src/inotifytools/inotify-nosys.h
index db76b2c..5f7b11b 100644
--- a/libinotifytools/src/inotifytools/inotify-nosys.h
+++ b/libinotifytools/src/inotifytools/inotify-nosys.h
@@ -100,8 +100,8 @@ struct inotify_event {
 # endif
 # if _MIPS_SIM == _MIPS_SIM_ABI64
 #  define __NR_inotify_init (__NR_Linux + 243)
-#  define __NR_inotify_add_watch (__NR_Linux + 243)
-#  define __NR_inotify_rm_watch (__NR_Linux + 243)
+#  define __NR_inotify_add_watch (__NR_Linux + 244)
+#  define __NR_inotify_rm_watch (__NR_Linux + 245)
 # endif
 # if _MIPS_SIM == _MIPS_SIM_NABI32
 #  define __NR_inotify_init (__NR_Linux + 247)
-- 
1.7.10.4

