# This file lists all frequencies used in Western Europe for DVB-T.
# The transmission parameters listed here are the ones generally used in
# Italy, broadcast neworks in other countries do use different parameters.
# Moreover, other countries use a bandwidth of 8 MHz also for Band III
# channels.
#
# Compiled in December 2010 by Marco d'Itri <md@linux.it>.
#
# References:
# http://en.wikipedia.org/wiki/Band_I#Europe
# http://en.wikipedia.org/wiki/Band_III#Europe
# http://en.wikipedia.org/wiki/File:VHF_Usage.svg
# http://en.wikipedia.org/wiki/Television_channel_frequencies


### VHF - Band III ###
# 5
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 177500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 6
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 184500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 7
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 191500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 8
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 198500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 9
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 205500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 212500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 11
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 219500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 12
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 226500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO


### UHF - Band IV ###
# 21
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 22
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 23
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 24
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 25
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 506000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 26
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 27
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 522000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 28
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 530000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 29
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 30
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 31
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 554000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 32
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 562000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 33
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 34
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 35
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 586000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 36
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 37
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO


### UHF - Band V ###
# 38
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 610000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 39
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 618000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 40
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 626000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 41
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 634000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 42
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 642000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 43
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 44
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 45
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 46
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 674000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 47
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 682000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 48
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 49
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 50
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 51
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 714000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 52
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 722000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 53
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 54
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 738000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 55
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 746000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 56
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 754000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 57
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 58
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 770000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 59
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 60
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 61
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 794000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 62
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 802000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 63
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 810000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 64
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 818000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 65
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 826000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 66
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 834000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 67
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 842000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 68
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

# 69
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 858000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

